{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":9,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMX-G"]
[]
[]
[]
[]
["","","","","","2AMX40G3V1B2","2AMX40G3V1B","2AMX50G3V1B2","2AMX50G3V1B"]
["Sound pressure level","Heating","","Nom.","dBA","48","48","50","50"]
["","Cooling","","Nom.","dBA","47","47","48","48"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","Screw bag","","","","1","1","1","1"]
["","Drain plug","","","","1","1","1","1"]
["","Air direction adjustment plate","","","","1","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","2.5","2.5","3.3","3.3"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","1.20","1.20","1.60","1.60"]
["","Type","","","","R-410A","R-410A","R-410A","R-410A"]
["Piping connections","Level difference","IU - IU","Max.","m","7.5","7.5","7.5","7.5"]
["","","IU - OU","Max.","m","15","15","15","15"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 20m)"]
["","Total piping length","System","Actual","m","30","30","30","30"]
["Dimensions","Unit","","Width","mm","765","765","765","765"]
["","","","Depth","mm","285","285","285","285"]
["","","","Height","mm","550","550","550","550"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","38","38","42","42"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; piping length: 5m"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases"]
["Standard Accessories","Reducer assembly","","","","","","1","1"]