{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":8,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMX-E"]
[]
[]
[]
[]
["","","","","","3AMX52E4V1B2","3AMX52E4V1B","3AMX52E3V1B"]
["Sound pressure level","Heating","","Nom.","dBA","47","47"]
["","Cooling","","Nom.","dBA","46","46"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Reducer assembly","","","","1","1","1"]
["","Air direction adjustment plate","","","","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","4.2","4.2"]
["","GWP","","","","2,087.5","2,087.5"]
["","Charge","","","kg","2.0","2.0"]
["","Type","","","","R-410A","R-410A"]
["Piping connections","Level difference","IU - IU","Max.","m","7.5","7.5"]
["","","IU - OU","Max.","m","15","15"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 30m)","0.02 (for piping length exceeding 30m)"]
["","Total piping length","System","Actual","m","50","50"]
["Dimensions","Unit","","Width","mm","936","936"]
["","","","Depth","mm","300","300"]
["","","","Height","mm","735","735"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","49","49"]
["Power supply","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","230","230"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 7.5m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 7.5m"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m"]
["","","","","","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases"]
["Dimensions","Unit","","Height","mm","","","735"]
["","","","Width","mm","","","936"]
["","","","Depth","mm","","","300"]
["Weight","Unit","","","kg","","","49"]
["Compressor","Type","","","","","","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","","","-10"]
["","","","Max.","°CDB","","","46"]
["","Heating","Ambient","Min.","°CWB","","","-15"]
["","","","Max.","°CWB","","","15.5"]
["Sound pressure level","Cooling","","Nom.","dBA","","","46"]
["","Heating","","Nom.","dBA","","","47"]
["Refrigerant","Type","","","","","","R-410A"]
["","Charge","","","kg","","","2.0"]
["","Charge","","","tCO2Eq","","","4.2"]
["","GWP","","","","","","2087.5"]
["Piping connections","Piping length","OU - IU","Max.","m","","","25"]
["","Additional refrigerant charge","","","kg/m","","","0.02 (for piping length exceeding 30m)"]
["","Level difference","IU - OU","Max.","m","","","15"]
["","","IU - IU","Max.","m","","","7.5"]
["","Total piping length","System","Actual","m","","","50"]
["Power supply","Phase","","","","","","1~"]
["","Frequency","","","Hz","","","50"]
["","Voltage","","","V","","","230"]