{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-A / AZQS-BV1"]
[]
[]
[]
[]
["","","","","ABQ125AV1 / AZQS125B7V1B","ABQ140AV1 / AZQS140B7V1B"]
["Cooling capacity","Nom.","","kW","12.1","13.0"]
["Nominal efficiency","EER","","","2.91","3.01"]
["","Annual energy consumption","","kWh","2,079","2,159"]
["","COP","","","3.41","3.41"]
["","Energy labeling Directive","Cooling","","C","B"]
["","","Heating","","B","B"]
["Heating capacity","Nom.","","kW","13.5","15.5"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]