{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-A"]
[]
[]
[]
[]
["","","","","ABQ100AV1","ABQ71AV1","ABQ125AV1","ABQ140AV1"]
["Sound pressure level","Heating","High","dBA","51","41","52","53"]
["","","Nom.","dBA","48","38","50","50"]
["","","Low","dBA","45","34","47","47"]
["","Cooling","Super high","dBA","55","44","53","55"]
["","","Low","dBA","45","34","47","47"]
["","","High","dBA","51","41","52","53"]
["","","Nom.","dBA","48","38","50","50"]
["Piping connections","Liquid","OD","mm","9.52","9.52","9.52","9.52"]
["","Gas","OD","mm","15.88","15.88","15.88","15.88"]
["Sound power level","Cooling","","dBA","76","64","76","78"]
["","Heating","","dBA","76","64","76","78"]
["Dimensions","Unit","Width","mm","1,325","1,020","1,388","1,588"]
["","","Depth","mm","638","600","541","541"]
["","","Height","mm","305","285","378","378"]
["Weight","Unit","","kg","47.0","35.0","50.0","56.0"]
["Fan","External static pressure","High","Pa","96","53","126","120"]
["","","Nom.","Pa","78","38","109","90"]
["","","Low","Pa","61","25","92","69"]
["","","Super high","Pa","118","78","147","147"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Name","","","V1","V1","V1","V1"]
["","Frequency","","Hz","50","50","50","50"]
["","Voltage","","V","230","230","230","230"]