{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-A"]
[]
[]
[]
[]
["","","","","ADEQ71A7VEB","ADEQ100A7VEB","ADEQ125A7VEB"]
["Sound pressure level","Heating","High","dBA","37","39","41"]
["","","Low","dBA","33","34","35"]
["","Cooling","Low","dBA","33","34","35"]
["","","High","dBA","37","39","41"]
["Cooling capacity","Total capacity","Nom.","kW","6.8 (1)","9.5 (1)","12.1 (1)"]
["Piping connections","Liquid","OD","mm","9.52","9.52","9.52"]
["","Gas","OD","mm","15.9","15.9","15.9"]
["","Drain","","","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)"]
["Required ceiling void >","mm","","","350","350","350"]
["Power input","Cooling","Nom.","kW","0.350 (1)","0.350 (1)","0.350 (1)"]
["","Heating","Nom.","kW","0.350 (2)","0.350 (2)","0.350 (2)"]
["Sound power level","Cooling","","dBA","57","62","67"]
["Dimensions","Unit","Width","mm","1,000","1,400","1,400"]
["","","Depth","mm","700","700","700"]
["","","Height","mm","300","300","300"]
["Casing","Colour","","","Galvanised steel / Non painted.","Galvanised steel / Non painted.","Galvanised steel / Non painted."]
["Weight","Unit","","kg","34","45","45"]
["Drain-up height","mm","","","625","625","625"]
["Heating capacity","Total capacity","Nom.","kW","7.5 (2)","10.8 (2)","13.5 (2)"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["","","","","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat."]
["","","","","(4) - The sound pressure values are mentioned for a unit installed with rear suction.","(4) - The sound pressure values are mentioned for a unit installed with rear suction.","(4) - The sound pressure values are mentioned for a unit installed with rear suction."]
["","","","","(5) - PED unit category: Art3§3: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(5) - PED unit category: Art3§3: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(5) - PED unit category: Art3§3: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC"]