{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":12,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXS-G / ARXS-G"]
[]
[]
[]
[]
["","","","","ATXS20G2V1B / ARXS20G3V1B","ATXS20G2V1B / ARXS20G4V1B","ATXS25G2V1B / ARXS25G3V1B","ATXS25G2V1B / ARXS25G4V1B","ATXS35G2V1B / ARXS35G3V1B","ATXS35G2V1B / ARXS35G4V1B","ATXS50G2V1B / ARXS50G2V1B","ATXS50G2V1B / ARXS50G3V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.3","1.3","1.4","1.4","1.7","1.7"]
["","Max.","","kW","2.8","2.8","3.2","3.2","4.0","4.0","5.3","5.3"]
["","Nom.","","kW","2.0 (3)","2.0 (2)","2.5 (3)","2.5 (2)","3.5 (3)","3.5 (2)","5.0 (3)","5.0 (2)"]
["Space cooling","SEER","","","5.87","5.87","6.54","6.54","6.43","6.43","5.30","5.30"]
["","Annual energy consumption","","kWh/a","119","119","134","134","190","190","330","330"]
["","Capacity","Pdesign","kW","2.00","2.00","2.50","2.50","3.50","3.50","5.00","5.00"]
["","Energy efficiency class","","","A+","A+","A++","A++","A++","A++","A","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.70","2.70","2.80","2.80","3.60","3.60","4.60","4.60"]
["","SCOP/A","","","4.61","4.61","4.55","4.55","4.32","4.32","3.98","3.98"]
["","Energy efficiency class","","","A++","A++","A+","A+","A+","A+","A","A"]
["","Annual energy consumption","","kWh/a","819","819","860","860","1,166","1,167","1,616","1,617"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","9.5","9.5","9.5","9.5","12.7","12.7"]
["","Drain","OD","mm","18.0","18.0","18.0","18.0","18.0","18.0","18.0","18.0"]
["Nominal efficiency","EER","","","4.26","4.26","4.55","4.55","4.02","4.02","3.29","3.29"]
["","Annual energy consumption","","kWh","235","235","275","275","435","435","760","760"]
["","COP","","","4.29","4.29","4.53","4.53","4.17","4.17","3.69","3.69"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","2.7 (4)","2.7 (3)","3.4 (4)","3.4 (3)","4.0 (4)","4.0 (3)","5.8 (4)","5.8 (3)"]
["","Min.","","kW","1.3","1.3","1.3","1.3","1.4","1.4","1.7","1.7"]
["","Max.","","kW","4.3","4.3","4.7","4.7","5.2","5.2","6.5","6.5"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]