{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXS-K / ARXS-L"]
[]
[]
[]
[]
["","","","","ATXS25K2V1B / ARXS25L2V1B","ATXS35K2V1B / ARXS35L2V1B","ATXS50K2V1B / ARXS50L2V1B","ATXS50K3V1B / ARXS50L2V1B"]
["Cooling capacity","Min.","","kW","1.3 (2)","1.4 (2)","1.7 (2)","1.7"]
["","Max.","","kW","3.2 (2)","4.0 (2)","5.3 (2)","5.3"]
["","Nom.","","kW","2.5 (2)","3.5 (2)","5.00 (2)","5.00 (2)"]
["Space cooling","SEER","","","7.51","7.10","6.46","6.46"]
["","Annual energy consumption","","kWh/a","117","173","271","271"]
["","Capacity","Pdesign","kW","2.50","3.50","5.00","5.00"]
["","Energy efficiency class","","","A++","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.5","3.6","4.6","4.60"]
["","SCOP/A","","","4.68","4.61","4.00","4.00"]
["","Energy efficiency class","","","A++","A++","A+","A+"]
["","Annual energy consumption","","kWh/a","747","1,094","1,608","1,608"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","12.7","12.7"]
["","Drain","OD","mm","18","18","18","18"]
["Nominal efficiency","Annual energy consumption","","kWh","285","420","705","794"]
["","EER","","","4.39 (1)","4.17 (1)","3.55","3.15 (1)"]
["","COP","","","4.52 (1)","4.76 (1)","4.00","4.00 (1)"]
["","Energy labeling Directive","Cooling","","A","A","A","A"]
["","","Heating","","A","A","A","A"]
["Heating capacity","Nom.","","kW","2.8 (3)","4.00 (3)","5.80 (3)","5.80 (2)"]
["","Min.","","kW","1.3 (3)","1.4 (3)","1.7 (3)","1.7"]
["","Max.","","kW","4.7 (3)","5.2 (3)","6.5 (3)","6.5"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - 220V"]
["","","","","(4) - 220V","(4) - 220V","(4) - 220V","(4) - 230V"]
["","","","","(5) - 230V","(5) - 230V","(5) - 230V","(5) - 240V"]
["","","","","(6) - 240V","(6) - 240V","(6) - 240V"]
["","","","","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]