{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXS-K / ARXS-L3"]
[]
[]
[]
[]
["","","","","ATXS25K2V1B / ARXS25L3V1B","ATXS25K3V1B / ARXS25L3V1B","ATXS35K2V1B / ARXS35L3V1B","ATXS35K3V1B / ARXS35L3V1B"]
["Cooling capacity","Min.","","kW","","","","1.4"]
["","Max.","","kW","","","","4.0"]
["","Nom.","","kW","2.5","2.5 (2)","3.5","3.5 (2)"]
["Space cooling","SEER","","","7.51","7.51","7.10","7.10"]
["","Annual energy consumption","","kWh/a","117","117","173","173"]
["","Capacity","Pdesign","kW","2.50","2.50","3.50","3.50"]
["","Energy efficiency class","","","A++","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.50","2.50","3.60","3.60"]
["","SCOP/A","","","4.68","4.68","4.61","4.61"]
["","Energy efficiency class","","","A++","A++","A++","A++"]
["","Annual energy consumption","","kWh/a","747","747","1,094","1,094"]
["Piping connections","Liquid","OD","mm","","6.35","","6.35"]
["","Gas","OD","mm","","9.5","","9.5"]
["","Drain","OD","mm","","18","","18"]
["Nominal efficiency","Annual energy consumption","","kWh","301","301","473","473"]
["","EER","","","4.15","4.15 (1)","3.70","3.70 (1)"]
["","COP","","","4.52","4.52 (1)","4.76","4.76 (1)"]
["","Energy labeling Directive","Cooling","","A","A","A","A"]
["","","Heating","","A","A","A","A"]
["Heating capacity","Nom.","","kW","2.8","2.8 (2)","4.00","4.00 (2)"]
["","Min.","","kW","","1.3","","1.4"]
["","Max.","","kW","","4.7","","5.2"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","","(3) - 220V","","(3) - 220V"]
["","","","","","(4) - 230V","","(4) - 230V"]
["","","","","","(5) - 240V","","(5) - 240V"]