{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":76,"n_cols":12,"rows_kept":76,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXS-K"]
[]
[]
[]
[]
["","","","","","ATXS20K2V1B","ATXS20K3V1B","ATXS25K2V1B","ATXS25K3V1B","ATXS35K2V1B","ATXS35K3V1B","ATXS50K3V1B"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","7.0","7.0","7.0","7.0","8.5","8.5"]
["Sound pressure level","Cooling","","Nom.","dBA","32","32","33","33","37","37"]
["Fan","Air flow rate","Heating","Nom.","m³/min","8.0","8.0","8.0","8.0","9.3","9.3"]
["Power input","Cooling","","Nom.","kW","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","","0.040 (3) (2) (4), 0.040 (3) (2) (4), 0.040 (3) (2) (4)","","0.026 (3) (2) (4), 0.026 (3) (2) (4), 0.026 (3) (2) (4)"]
["","Heating","","Nom.","kW","0.040 (1) (3) (2), 0.040 (1) (3) (2), 0.040 (1) (3) (2)","","0.040 (2) (4) (3), 0.040 (2) (4) (3), 0.040 (2) (4) (3)","","0.028 (3) (2), 0.028 (3) (2), 0.280 (4)"]
["Casing","Colour","","","","White","White","White","White","White","White"]
["Dimensions","Unit","","Height","mm","289","289","289","289","298","298"]
["","","","Width","mm","780","780","780","780","900","900"]
["","","","Depth","mm","215","215","215","215","215","215"]
["Weight","Unit","","","kg","8","8","8","8","11","11"]
["Fan","Air flow rate","Cooling","High","m³/min","9.1","9.1","9.1","9.1","11.2","11.2"]
["","","","Low","m³/min","5.0","5.0","5.0","5.0","5.8","5.8"]
["","","","Silent operation","m³/min","3.9","3.9","3.9","3.9","4.1","4.1"]
["","","Heating","High","m³/min","10.0","10.0","10.0","10.0","12.1","12.1"]
["","","","Low","m³/min","6.0","6.0","6.0","6.0","6.5","6.5"]
["","","","Silent operation","m³/min","4.3","4.3","4.3","4.3","4.2","4.2"]
["Sound power level","Cooling","","","dBA","54","56","58","58","59","59"]
["","Heating","","","dBA","56","56","58","58","59","59"]
["Sound pressure level","Cooling","","High","dBA","40","40","41","41","45","45"]
["","","","Low","dBA","24","24","25","25","29","29"]
["","","","Silent operation","dBA","19","19","19","19","19","19"]
["","Heating","","High","dBA","40","40","41","41","45","45"]
["","","","Low","dBA","27","27","27","27","29","29"]
["","","","Silent operation","dBA","19","19","19","19","19","19"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.5","9.5","9.5","9.5","9.5","9.5"]
["","Drain","","","","18","18","18","18","18","18"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","Operation manual","","","","1","1","1","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1","1"]
["","Titanium apatite photocatalytic air purification filter","","","","2","2","2","2","2","2","2"]
["Power supply","Name","","","","V1","V1","V1","V1","V1","V1"]
["","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - SL: The silent fan level of the air flow rate setting"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected."]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 220V"]
["Sound pressure level","Heating","","Nom.","dBA","","34","34","34","39","39"]
["Control systems","Infrared remote control","","","","","ARC466A6","","ARC466A6","","ARC466A9"]
["Standard Accessories","Batteries","","","","","","","","2","2","2"]
["Sound pressure level","Heating","","High","dBA","","","","","","","47"]
["","","","Silent operation","dBA","","","","","","","24"]
["","","","Low","dBA","","","","","","","34"]
["","Cooling","","Silent operation","dBA","","","","","","","23"]
["","","","Low","dBA","","","","","","","34"]
["","","","High","dBA","","","","","","","46"]
["","","","Nom.","dBA","","","","","","","40"]
["","Cooling","","Nom.","dBA","","","","","","","40"]
["Control systems","Infrared remote control","","","","","","","","","","ARC466A9"]
["Piping connections","Liquid","","OD","mm","","","","","","","6.35"]
["","Gas","","OD","mm","","","","","","","12.7"]
["","Drain","","","","","","","","","","18"]
["Sound power level","Cooling","","","dBA","","","","","","","60"]
["","Heating","","","dBA","","","","","","","60"]
["Dimensions","Unit","","Width","mm","","","","","","","900"]
["","","","Depth","mm","","","","","","","215"]
["","","","Height","mm","","","","","","","298"]
["Casing","Colour","","","","","","","","","","White"]
["Weight","Unit","","","kg","","","","","","","11"]
["Power supply","Phase","","","","","","","","","","1~"]
["","Name","","","","","","","","","","V1"]
["","Frequency","","","Hz","","","","","","","50"]
["","Voltage","","","V","","","","","","","220-240"]
["Notes","","","","","","","","","","","(4) - 230V"]
["","","","","","","","","","","","(5) - 240V"]