{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXG-J-S"]
[]
[]
[]
[]
["","","","","","CTXG50JV1BS"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","8.7"]
["Sound pressure level","Cooling","","Nom.","dBA","41"]
["Fan","Air flow rate","Heating","Nom.","m³/min","9.8"]
["Sound pressure level","Heating","","Nom.","dBA","41"]
["Power input","Cooling","","Nom.","kW","0.032"]
["","Heating","","Nom.","kW","0.038"]
["Casing","Colour","","","","Silver"]
["Dimensions","Unit","","Height","mm","295"]
["","","","Width","mm","915"]
["","","","Depth","mm","155"]
["Weight","Unit","","","kg","11"]
["Fan","Air flow rate","Cooling","High","m³/min","10.5"]
["","","","Low","m³/min","6.9"]
["","","","Silent operation","m³/min","5.9"]
["","","Heating","High","m³/min","11.4"]
["","","","Low","m³/min","8.1"]
["","","","Silent operation","m³/min","7.1"]
["Sound power level","Cooling","","","dBA","60"]
["","Heating","","","dBA","60"]
["Sound pressure level","Cooling","","High","dBA","44"]
["","","","Low","dBA","35"]
["","","","Silent operation","dBA","32"]
["","Heating","","High","dBA","44"]
["","","","Low","dBA","35"]
["","","","Silent operation","dBA","32"]
["Piping connections","Liquid","","OD","mm","6.35"]
["","Gas","","OD","mm","12.7"]
["","Drain","","","","18"]
["Standard Accessories","Installation manual","","","","1"]
["","Operation manual","","","","1"]
["","Batteries","","","","2"]
["","Indoor unit fixing screws","","","","2"]
["","Infrared remote control","","","","1"]
["","Mounting plate","","","","1"]
["","Paper pattern for installation","","","","2"]
["","Remote control holder","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","2"]
["Power supply","Name","","","","V1"]
["","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - 220V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240V"]