{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXG-J-W"]
[]
[]
[]
[]
["","","","","CTXG50JV1BW"]
["Sound pressure level","Heating","High","dBA","44"]
["","","Silent operation","dBA","32"]
["","","Low","dBA","35"]
["","Cooling","Silent operation","dBA","32"]
["","","Low","dBA","35"]
["","","High","dBA","44"]
["","","Nom.","dBA","41"]
["","Cooling","Nom.","dBA","41"]
["Standard Accessories","Titanium apatite photocatalytic air purification filter","","","2"]
["","Operation manual","","","1"]
["","Installation manual","","","1"]
["","Infrared remote control","","","1"]
["","Batteries","","","2"]
["","Remote control holder","","","1"]
["","Indoor unit fixing screws","","","2"]
["","Mounting plate","","","1"]
["","Paper pattern for installation","","","2"]
["Piping connections","Liquid","OD","mm","6.35"]
["","Gas","OD","mm","12.7"]
["","Drain","","","18"]
["Power input","Cooling","Nom.","kW","0.032"]
["","Heating","Nom.","kW","0.038"]
["Sound power level","Cooling","","dBA","60"]
["","Heating","","dBA","60"]
["Dimensions","Unit","Width","mm","915"]
["","","Depth","mm","155"]
["","","Height","mm","295"]
["Casing","Colour","","","White"]
["Weight","Unit","","kg","11"]
["Power supply","Phase","","","1~"]
["","Name","","","V1"]
["","Frequency","","Hz","50"]
["","Voltage","","V","220-240"]
["Notes","","","","(1) - 220V"]
["","","","","(2) - 230V"]
["","","","","(3) - 240V"]
["","","","","(4) - SL: The silent fan level of the air flow rate setting"]
["","","","","(5) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected."]