{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":11,"n_cols":10,"rows_kept":11,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBH-C / ERHQ-BW1"]
[]
[]
[]
[]
["","","","","EHBH16CA3V / ERHQ011BAW1","EHBH16CA9W / ERHQ011BAW1","EHBH16CA3V / ERHQ014BAW1","EHBH16CA9W / ERHQ014BAW1","EHBH16CA3V / ERHQ016BAW1","EHBH16CA9W / ERHQ016BAW1"]
["COP","","","","4.30 (1), 3.39 (2)","4.30 (1), 3.39 (2)","4.24 (1), 3.22 (2)","4.24 (1), 3.22 (2)","4.20 (1), 3.22 (2)","4.20 (1), 3.22 (2)"]
["Heating capacity","Nom.","","kW","11.32 (1), 10.98 (2)","11.32 (1), 10.98 (2)","14.50 (1), 13.57 (2)","14.50 (1), 13.57 (2)","16.05 (1), 15.11 (2)","16.05 (1), 15.11 (2)"]
["Power input","Heating","Nom.","kW","2.63 (1), 3.24 (2)","2.63 (1), 3.24 (2)","3.42 (1), 4.21 (2)","3.42 (1), 4.21 (2)","3.82 (1), 4.69 (2)","3.82 (1), 4.69 (2)"]
["Notes","","","","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)"]
["","","","","(2) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]