{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":10,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBH-C / ERLQ-CW1"]
[]
[]
[]
[]
["","","","","EHBH16CA3V / ERLQ011CAW1","EHBH16CA9W / ERLQ011CAW1","EHBH16CA3V / ERLQ014CAW1","EHBH16CA9W / ERLQ014CAW1","EHBH16CA3V / ERLQ016CAW1","EHBH16CA9W / ERLQ016CAW1"]
["COP","","","","4.6 (1), 2.75 (3), 3.55 (2), 2.10 (4)","4.6 (1), 2.75 (3), 3.55 (2), 2.10 (4)","4.3 (1), 2.65 (3), 3.32 (2), 2.08 (4)","4.3 (1), 2.65 (3), 3.32 (2), 2.08 (4)","4.25 (1), 2.64 (3), 3.26 (2), 2.09 (4)","4.25 (1), 2.64 (3), 3.26 (2), 2.09 (4)"]
["Heating capacity","Nom.","","kW","11.2 (1), 11.00 (2)","11.2 (1), 11.00 (2)","14.5 (1), 13.60 (2)","14.5 (1), 13.60 (2)","16 (1), 15.20 (2)","16 (1), 15.20 (2)"]
["","Max.","","kW","8.6 (3), 8.60 (4)","8.6 (3), 8.60 (4)","10.6 (3), 10.80 (4)","10.6 (3), 10.80 (4)","11.4 (3), 10.90 (4)","11.4 (3), 10.90 (4)"]
["Power input","Heating","Max.","kW","3.13 (3), 4.10 (4)","3.13 (3), 4.10 (4)","4.00 (3), 5.19 (4)","4.00 (3), 5.19 (4)","4.32 (3), 5.22 (4)","4.32 (3), 5.22 (4)"]
["","","Nom.","kW","2.43 (1), 3.10 (2)","2.43 (1), 3.10 (2)","3.37 (1), 4.10 (2)","3.37 (1), 4.10 (2)","3.76 (1), 4.66 (2)","3.76 (1), 4.66 (2)"]
["Notes","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["","","","","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C"]
["","","","","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C"]