{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":10,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBH-C"]
[]
[]
[]
[]
["","","","","","EHBH04CA3V","EHBH08CA3V","EHBH08CA9W","EHBH16CA3V","EHBH16CA9W"]
["Sound pressure level","Nom.","","","dBA","26","26","26","33","33"]
["Water side Heat exchanger","Water flow rate","Heating","Max.","l/min","25","34","34","51","51"]
["Operation range","Heating","Water side","Max.","°C","55 (4)","55 (4)","55 (4)","55 (4)","55 (4)"]
["","","","Min.","°C","15 (4)","15 (4)","15 (4)","15 (4)","15 (4)"]
["Sound power level","Nom.","","","dBA","40 (12)","40 (12)","40 (12)","47 (12)","47 (12)"]
["Dimensions","Unit","","Width","mm","480","480","480","480","480"]
["","","","Depth","mm","344","344","344","344","344"]
["","","","Height","mm","890","890","890","890","890"]
["Casing","Material","","","","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal"]
["","Colour","","","","White","White","White","White","White"]
["Weight","Unit","","","kg","44","46","48","47","48"]
["PED","Category","","","","Art3§3","Category I","Category I","Art3§3","Art3§3"]
["Wiring connections","For connection with user interface","","Remark","","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)"]
["","","","Quantity","","2","2","2","2","2"]
["Notes","","","","","(1) - With option kit *KHBDP installed: Height = XXX mm","(1) - With option kit *KHBDP installed: Height = XXX mm","(1) - With option kit *KHBDP installed: Height = XXX mm","(1) - With option kit *KHBDP installed: Height = XXX mm","(1) - With option kit *KHBDP installed: Height = XXX mm"]
["","","","","","(2) - The sound pressure level is measured via a microphone at a 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.","(2) - The sound pressure level is measured via a microphone at a 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.","(2) - The sound pressure level is measured via a microphone at a 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.","(2) - The sound pressure level is measured via a microphone at a 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.","(2) - The sound pressure level is measured via a microphone at a 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment."]
["","","","","","(3) - The sound pressure level mentioned is maximum possible value inside operation range of unit","(3) - The sound pressure level mentioned is maximum possible value inside operation range of unit","(3) - The sound pressure level mentioned is maximum possible value inside operation range of unit","(3) - The sound pressure level mentioned is maximum possible value inside operation range of unit","(3) - The sound pressure level mentioned is maximum possible value inside operation range of unit"]
["","","","","","(4) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(4) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(4) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(4) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(4) - 15°C-25°C: BUH only, no heat pump operation = during commissioning"]
["","","","","","(5) - Including piping + PHE + back-up heater; excluding expansion vessel","(5) - Including piping + PHE + back-up heater; excluding expansion vessel","(5) - Including piping + PHE + back-up heater; excluding expansion vessel","(5) - Including piping + PHE + back-up heater; excluding expansion vessel","(5) - Including piping + PHE + back-up heater; excluding expansion vessel"]
["","","","","","(6) - Water circuit piping connections diameter is connection after ball valves, Connection at unit is G1-1/4 FEMALE","(6) - Water circuit piping connections diameter is connection after ball valves, Connection at unit is G1-1/4 FEMALE","(6) - Water circuit piping connections diameter is connection after ball valves, Connection at unit is G1-1/4 FEMALE","(6) - Water circuit piping connections diameter is connection after ball valves, Connection at unit is G1-1/4 FEMALE","(6) - Water circuit piping connections diameter is connection after ball valves, Connection at unit is G1-1/4 FEMALE"]
["","","","","","(7) - See separate drawing for operation range","(7) - See separate drawing for operation range","(7) - See separate drawing for operation range","(7) - See separate drawing for operation range","(7) - See separate drawing for operation range"]
["","","","","","(8) - > 50°C BSH only, no heatpump operation","(8) - > 50°C BSH only, no heatpump operation","(8) - > 50°C BSH only, no heatpump operation","(8) - > 50°C BSH only, no heatpump operation","(8) - > 50°C BSH only, no heatpump operation"]
["","","","","","(9) - BUH 3V/9W can only operate at flow > 12/15 l/min","(9) - BUH 3V/9W can only operate at flow > 12/15 l/min","(9) - BUH 3V/9W can only operate at flow > 12/15 l/min","(9) - BUH 3V/9W can only operate at flow > 12/15 l/min","(9) - BUH 3V/9W can only operate at flow > 12/15 l/min"]
["","","","","","(10) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models","(10) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models","(10) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models","(10) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models","(10) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models"]
["","","","","","(11) - PED unit category: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(11) - PED unit category: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(11) - PED unit category: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(11) - PED unit category: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(11) - PED unit category: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC"]
["","","","","","(12) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(12) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(12) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(12) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(12) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)"]