{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":10,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBX-C"]
[]
[]
[]
[]
["","","","","","EHBX04CA3V","EHBX08CA3V","EHBX08CA9W","EHBX16CA9W","EHBX16CA3V"]
["Casing","Colour","","","","White","White","White","White","White"]
["","Material","","","","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal"]
["Dimensions","Unit","","Height","mm","890","890","890","890","890"]
["","","","Width","mm","480","480","480","480","480"]
["","","","Depth","mm","344","344","344","344","344"]
["Weight","Unit","","","kg","44","46","48","48","47"]
["PED","Category","","","","Art3§3","Category I","Category I","Art3§3","Art3§3"]
["Water side Heat exchanger","Water flow rate","Heating","Max.","l/min","25","34","34","51","51"]
["","","Cooling","Max.","l/min","25","34","34","51","51"]
["Sound power level","Nom.","","","dBA","40","40","40","47","47"]
["Sound pressure level","Nom.","","","dBA","26","26","26","33","33"]
["Operation range","Heating","Water side","Min.","°C","15","15","15","15","15"]
["","","","Max.","°C","55","55","55","55","55"]
["","Cooling","Ambient","Min.","°CDB","10","10","10","10","10"]
["","","Water side","Min.","°C","5","5","5","5","5"]
["","","","Max.","°C","22","22","22","22","22"]
["Wiring connections","For connection with user interface","","Quantity","","2","2","2","2","2"]
["","","","Remark","","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)"]
["Notes","","","","","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(1) - 15°C-25°C: BUH only no heat pump operation = during commissioning","(1) - 15°C-25°C: BUH only no heat pump operation = during commissioning"]
["","","","","","(2) - 15°C-25°C: BUH only no heat pump operation = during commissioning","(2) - 15°C-25°C: BUH only no heat pump operation = during commissioning","(2) - 15°C-25°C: BUH only no heat pump operation = during commissioning","(2) - Including piping + PHE + back-up heater; excluding expansion vessel","(2) - Including piping + PHE + back-up heater; excluding expansion vessel"]
["","","","","","(3) - Including piping + PHE + back-up heater; excluding expansion vessel","(3) - Including piping + PHE + back-up heater; excluding expansion vessel","(3) - Including piping + PHE + back-up heater; excluding expansion vessel","(3) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models","(3) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models"]