{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":9,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSH-A"]
[]
[]
[]
[]
["","","","","","EHSH04P30AA","EHSH08P30AA","EHSH08P50AA","EHSH16P50AA"]
["Sound pressure level","Nom.","","","dBA","28","28","28","28"]
["Refrigerant","Charge","","","kg","1.5","1.6","1.6","3.4"]
["","Type","","","","R-410A","R-410A","R-410A","R-410A"]
["Operation range","Heating","Water side","Max.","°C","55","55","55","55"]
["","","","Min.","°C","15 (10)","15 (10)","15 (10)","15 (10)"]
["Sound power level","Nom.","","","dBA","40","40","40","40"]
["Dimensions","Unit","","Width","mm","615","615","790","790"]
["","","","Depth","mm","595","595","790","790"]
["","","","Height","mm","1,945","1,945","1,945","1,945"]
["Casing","Material","","","","Impact resistant polypropylene","Impact resistant polypropylene","Impact resistant polypropylene","Impact resistant polypropylene"]
["","Colour","","","","Traffic white (RAL9016) / Dark grey (RAL7011)","Traffic white (RAL9016) / Dark grey (RAL7011)","Traffic white (RAL9016) / Dark grey (RAL7011)","Traffic white (RAL9016) / Dark grey (RAL7011)"]
["Weight","Unit","","","kg","87","87","114","116"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Name","","","","V3","V3","V3","please refer to outdoor unit"]
["","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","230","230","230","230"]
["Electric heater","Power supply","","Frequency","Hz","50","50","50","50"]
["","","","Name","","3V / 9W","3V / 9W","3V / 9W","3V / 9W"]
["","","","Phase","","1~ / 3~","1~ / 3~","1~ / 3~","1~ / 3~"]
["Current","Recommended fuses","","","A","20","20","20","20"]
["Notes","","","","","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","","(5) - Heat up of tank only with heat pump, no electrical heater","(5) - Heat up of tank only with heat pump, no electrical heater","(5) - Heat up of tank only with heat pump, no electrical heater","(5) - Heat up of tank only with heat pump, no electrical heater"]
["","","","","","(6) - For tapping volume 140l -> 5820 Wh (bath) / 8kW heat pump","(6) - For tapping volume 140l -> 5820 Wh (bath) / 8kW heat pump","(6) - For tapping volume 140l -> 5820 Wh (bath) / 8kW heat pump","(6) - For tapping volume 140l -> 5820 Wh (bath) / 8kW heat pump"]
["","","","","","(7) - For tapping volume 90l -> 3660 Wh (bath) / 8kW heat pump","(7) - For tapping volume 90l -> 3660 Wh (bath) / 8kW heat pump","(7) - For tapping volume 90l -> 3660 Wh (bath) / 8kW heat pump","(7) - For tapping volume 90l -> 3660 Wh (bath) / 8kW heat pump"]
["","","","","","(8) - For tapping volume 140l -> 5820 Wh (bath) / 16kW heat pump","(8) - For tapping volume 140l -> 5820 Wh (bath) / 16kW heat pump","(8) - For tapping volume 140l -> 5820 Wh (bath) / 16kW heat pump","(8) - For tapping volume 140l -> 5820 Wh (bath) / 16kW heat pump"]
["","","","","","(9) - For tapping volume 90l -> 3660 Wh (bath) / 16kW heat pump","(9) - For tapping volume 90l -> 3660 Wh (bath) / 16kW heat pump","(9) - For tapping volume 90l -> 3660 Wh (bath) / 16kW heat pump","(9) - For tapping volume 90l -> 3660 Wh (bath) / 16kW heat pump"]
["","","","","","(10) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(10) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(10) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(10) - 15°C-25°C: BUH only, no heat pump operation = during commissioning"]