{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":12,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-A / ERLQ-CV3"]
[]
[]
[]
[]
["","","","","","EHSX08P30AA / ERLQ006CAV3","EHSX08P50AA / ERLQ006CAV3","EHSX08P30AA / ERLQ008CAV3","EHSX08P50AA / ERLQ008CAV3","EHSX16P50AA / ERLQ011CAV3","EHSX16P50AA / ERLQ014CAV3","EHSX16P50AA / ERLQ016CAV3"]
["Domestic hot water heating","General","","Declared load profile","","L","XL","L","XL","XL","XL","XL"]
["","Average climate","","Water heating energy efficiency class","","A","A","A","A","A","A","A"]
["COP","","","","","4.65 (1), 3.66 (2), 2.73 (3), 3.64 (4)","4.65 (1), 3.66 (2), 2.73 (3), 3.64 (4)","4.60 (1), 3.57 (2), 2.78 (3), 3.54 (4)","4.60 (1), 3.57 (2), 2.78 (3), 3.54 (4)","4.38 (1), 3.32 (2), 2.45 (3), 3.29 (4)","4.27 (1), 3.34 (2), 2.58 (3), 3.22 (4)","4.10 (1), 3.22 (2), 2.44 (3), 3.15 (4)"]
["Indoor unit","","","","","EHSX08P30AA","EHSX08P50AA","EHSX08P30AA","EHSX08P50AA","EHSX16P50AA","EHSX16P50AA","EHSX16P50AA"]
["Space heating","Average climate water outlet 55°C","General","Seasonal space heating eff. class","","A++","A++","A++","A++","A++","A++","A++"]
["Cooling capacity","Nom.","","","kW","5.2 (1), 4.6 (2)","5.2 (1), 4.6 (2)","5.2 (1), 4.6 (2)","5.2 (1), 4.6 (2)","15.1 (1), 11.7 (2)","16.1 (1), 12.6 (2)","16.8 (1), 13.1 (2)"]
["","Min.","","","kW","2.5 (1), 2.6 (2)","2.5 (1), 2.6 (2)","2.5 (1), 2.6 (2)","2.5 (1), 2.6 (2)","2.5 (1), 2.6 (2)","2.5 (1), 2.6 (2)"]
["","Max.","","","kW","7.3 (1), 5.5 (2)","7.3 (1), 5.5 (2)","8.4 (1), 6.4 (2)","8.4 (1), 6.4 (2)","15.1 (1), 11.7 (2)","16.1 (1), 12.6 (2)","16.8 (1), 13.1 (2)"]
["EER","","","","","3.65 (1), 2.51 (2)","3.65 (1), 2.51 (2)","3.65 (1), 2.51 (2)","3.65 (1), 2.51 (2)","3.32 (1), 2.72 (2)","2.96 (1), 2.47 (2)","2.72 (1), 2.29 (2)"]
["Heating capacity","Nom.","","","kW","6.06 (1), 5.78 (2), 5.14 (3), 4.60 (4)","6.06 (1), 5.78 (2), 5.14 (3), 4.60 (4)","7.78 (1), 7.27 (2), 5.53 (3), 5.51 (4)","7.78 (1), 7.27 (2), 5.53 (3), 5.51 (4)","11.80 (1), 10.40 (2), 5.95 (3), 7.74 (4)","14.81 (1), 13.73 (2), 8.28 (3), 9.57 (4)","15.34 (1), 14.86 (2), 8.04 (3), 10.05 (4)"]
["","Min.","","","kW","1.80 (1), 1.81 (2)","1.80 (1), 1.81 (2)","1.80 (1), 1.81 (2)","1.80 (1), 1.81 (2)"]
["","Max.","","","kW","8.35 (1), 7.95 (2)","8.35 (1), 7.95 (2)","10.02 (1), 9.53 (2)","10.02 (1), 9.53 (2)","11.38 (1), 11.00 (2)","14.55 (1), 13.59 (2)","16.10 (1), 15.22 (2)"]
["Power input","Heating","","Max.","kW","1.99 (1), 2.32 (2)","1.99 (1), 2.32 (2)","2.54 (1), 2.96 (2)","2.54 (1), 2.96 (2)","2.64 (1), 3.25 (2)","3.43 (1), 4.22 (2)","3.83 (1), 4.71 (2)"]
["","","","Nom.","kW","1.30 (1), 1.58 (2), 1.88 (3), 1.26 (4)","1.30 (1), 1.58 (2), 1.88 (3), 1.26 (4)","1.69 (1), 2.04 (2), 1.98 (3), 1.56 (4)","1.69 (1), 2.04 (2), 1.98 (3), 1.56 (4)","2.57 (1), 3.13 (2), 2.43 (3), 2.35 (4)","3.42 (1), 4.07 (2), 3.17 (3), 2.93 (4)","3.42 (1), 4.07 (2), 3.17 (3), 2.93 (4)"]
["","Cooling","","Nom.","kW","1.43 (1), 1.85 (2)","1.43 (1), 1.85 (2)","1.43 (1), 1.85 (2)","1.43 (1), 1.85 (2)","4.55 (1), 4.30 (2)","5.44 (1), 5.10 (2)","6.18 (1), 5.72 (2)"]
["","","","Max.","kW","2.27 (1), 2.51 (2)","2.27 (1), 2.51 (2)","2.89 (1), 3.20 (2)","2.89 (1), 3.20 (2)","4.53 (1), 4.31 (2)","5.42 (1), 5.09 (2)","6.15 (1), 5.74 (2)"]
["Notes","","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["","","","","","(3) - EW 30°C; LW 35°C; ambient conditions: -7°CDB/-8°CWB","(3) - EW 30°C; LW 35°C; ambient conditions: -7°CDB/-8°CWB","(3) - EW 30°C; LW 35°C; ambient conditions: -7°CDB/-8°CWB","(3) - EW 30°C; LW 35°C; ambient conditions: -7°CDB/-8°CWB","(3) - EW 30°C; LW 35°C; ambient conditions: -7°CDB/-8°CWB","(3) - EW 30°C; LW 35°C; ambient conditions: -7°CDB/-8°CWB","(3) - EW 30°C; LW 35°C; ambient conditions: -7°CDB/-8°CWB"]
["","","","","","(4) - EW 30°C; LW 35°C; ambient conditions: 2°CDB/1°CWB","(4) - EW 30°C; LW 35°C; ambient conditions: 2°CDB/1°CWB","(4) - EW 30°C; LW 35°C; ambient conditions: 2°CDB/1°CWB","(4) - EW 30°C; LW 35°C; ambient conditions: 2°CDB/1°CWB","(4) - EW 30°C; LW 35°C; ambient conditions: 2°CDB/1°CWB","(4) - EW 30°C; LW 35°C; ambient conditions: 2°CDB/1°CWB","(4) - EW 30°C; LW 35°C; ambient conditions: 2°CDB/1°CWB"]
["","","","","","(5) - Tamb 35°C - LWE 18°C (DT=5°C)","(5) - Tamb 35°C - LWE 18°C (DT=5°C)","(5) - Tamb 35°C - LWE 18°C (DT=5°C)","(5) - Tamb 35°C - LWE 18°C (DT=5°C)","(5) - Tamb 35°C - LWE 18°C (DT=5°C)","(5) - Tamb 35°C - LWE 18°C (DT=5°C)","(5) - Tamb 35°C - LWE 18°C (DT=5°C)"]
["","","","","","(6) - Tamb 35°C - LWE 7°C (DT=5°C)","(6) - Tamb 35°C - LWE 7°C (DT=5°C)","(6) - Tamb 35°C - LWE 7°C (DT=5°C)","(6) - Tamb 35°C - LWE 7°C (DT=5°C)","(6) - Tamb 35°C - LWE 7°C (DT=5°C)","(6) - Tamb 35°C - LWE 7°C (DT=5°C)","(6) - Tamb 35°C - LWE 7°C (DT=5°C)"]
["","","","","","(7) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(7) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(7) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(7) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(7) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(7) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(7) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)"]
["","","","","","(8) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(8) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(8) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(8) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(8) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(8) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(8) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]