{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVH-C3VF"]
[]
[]
[]
[]
["","","","","","EHVH04S18CA3VF","EHVH08S18CA3VF"]
["Sound pressure level","Nom.","","","dBA","28","28"]
["Water side Heat exchanger","Water flow rate","Heating","Max.","l/min","25","34"]
["Operation range","Heating","Water side","Max.","°C","55 (5)","55 (5)"]
["","","","Min.","°C","15 (5)","15 (5)"]
["Sound power level","Nom.","","","dBA","42 (2)","42 (2)"]
["Dimensions","Unit","","Width","mm","600","600"]
["","","","Depth","mm","728","728"]
["","","","Height","mm","1,732","1,732"]
["Casing","Material","","","","Precoated sheet metal","Precoated sheet metal"]
["","Colour","","","","White","White"]
["Weight","Unit","","","kg","120","121"]
["PED","Category","","","","Art3§3","Category I"]
["Wiring connections","For connection with user interface","","Remark","","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)"]
["","","","Quantity","","2","2"]
["Electric heater","Current back-up heater","","Running current","A","13","13"]
["","Power supply","","Frequency","Hz","50","50"]
["","","","Voltage","V","230","230"]
["","","","Phase","","1~","1~"]
["Notes","","","","","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897"]
["","","","","","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)"]
["","","","","","(3) - The sound pressure level is measured via a microphone at a 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.","(3) - The sound pressure level is measured via a microphone at a 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment."]
["","","","","","(4) - The sound pressure level mentioned is valid for pump medium speed - 0 ESP / medium speed - nominal flow / high speed - nominal flow","(4) - The sound pressure level mentioned is valid for pump medium speed - 0 ESP / medium speed - nominal flow / high speed - nominal flow"]
["","","","","","(5) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(5) - 15°C-25°C: BUH only, no heat pump operation = during commissioning"]
["","","","","","(6) - Including piping + PHE + back-up heater; excluding expansion vessel","(6) - Including piping + PHE + back-up heater; excluding expansion vessel"]
["","","","","","(7) - Water circuit piping connections diameter is connection after ball valves, Connection at unit is G1-1/4 FEMALE","(7) - Water circuit piping connections diameter is connection after ball valves, Connection at unit is G1-1/4 FEMALE"]
["","","","","","(8) - See separate drawing for operation range","(8) - See separate drawing for operation range"]
["","","","","","(9) - For *RLQ* outdoor units >55°C BUH only, no heatpump operation","(9) - For *RLQ* outdoor units >55°C BUH only, no heatpump operation"]
["","","","","","(10) - Minimum flow is mentioned for heat pump operation. To allow backup heater to operate safely a higher minimum flow is required:12 l/min","(10) - Minimum flow is mentioned for heat pump operation. To allow backup heater to operate safely a higher minimum flow is required:12 l/min"]
["","","","","","(11) - Above mentioned power supply of the hydrobox is for the backup heater only. The switch box and the pump of the hydrobox are supplied via the outdoor unit.","(11) - Above mentioned power supply of the hydrobox is for the backup heater only. The switch box and the pump of the hydrobox are supplied via the outdoor unit."]
["","","","","","(12) - For more details on current & voltage range, refer to the installation manual.","(12) - For more details on current & voltage range, refer to the installation manual."]
["","","","","","(13) - PED unit category: Art3§3: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(13) - PED unit category: Art3§3: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC"]