{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":12,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVH-CB"]
[]
[]
[]
[]
["","","","","","EHVH04S18CB3V","EHVH08S18CB3V","EHVH08S26CB9W","EHVH11S26CB9W","EHVH11S18CB3V","EHVH16S26CB9W","EHVH16S18CB3V"]
["Sound pressure level","Nom.","","","dBA","","28.0 (7)"]
["Sound power level","Nom.","","","dBA","","42.0 (6)"]
["Dimensions","Unit","","Width","mm","","600"]
["","","","Depth","mm","","728"]
["","","","Height","mm","","1,732"]
["Casing","Material","","","","","Precoated sheet metal"]
["","Colour","","","","","White"]
["Weight","Unit","","","kg","","117"]
["PED","Category","","","","","Category I, See note 1"]
["Wiring connections","For connection with user interface","","Remark","","","0.75 mm² till 1.25 mm² (max length 500m)"]
["","","","Quantity","","","2"]
["Power supply","Name","","","","","See note 14"]
["Electric heater","Power supply","","Frequency","Hz","","50"]
["","","","Voltage","V","","230"]
["","","","Name","","","3V3"]
["","","","Phase","","","1~"]
["Notes","","","","","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(1) - PED unit category: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation)."]
["","","","","","(2) - Based on a dT of 45 K","(2) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(2) - Based on a dT of 45 K","(2) - Based on a dT of 45 K","(2) - Based on a dT of 45 K","(2) - Based on a dT of 45 K","(2) - Based on a dT of 45 K"]
["","","","","","(3) - Including piping + PHE + back-up heater; excluding expansion vessel","(3) - Based on a dT of 45 K","(3) - Including piping + PHE + back-up heater; excluding expansion vessel","(3) - Including piping + PHE + back-up heater; excluding expansion vessel","(3) - Including piping + PHE + back-up heater; excluding expansion vessel","(3) - Including piping + PHE + back-up heater; excluding expansion vessel","(3) - Including piping + PHE + back-up heater; excluding expansion vessel"]
["","","","","","(4) - Excluding the water in the unit. This minimum water volume is sufficient for most applications. During critical processes extra water may be required.","(4) - Including piping + PHE + back-up heater; excluding expansion vessel","(4) - Excluding the water in the unit. This minimum water volume is sufficient for most applications. During critical processes extra water may be required.","(4) - Excluding the water in the unit. This minimum water volume is sufficient for most applications. During critical processes extra water may be required.","(4) - Excluding the water in the unit. This minimum water volume is sufficient for most applications. During critical processes extra water may be required.","(4) - Excluding the water in the unit. This minimum water volume is sufficient for most applications. During critical processes extra water may be required.","(4) - Excluding the water in the unit. This minimum water volume is sufficient for most applications. During critical processes extra water may be required."]
["","","","","","(5) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(5) - Excluding the water in the unit. This minimum water volume is sufficient for most applications. During critical processes extra water may be required.","(5) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(5) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(5) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(5) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(5) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)"]
["","","","","","(6) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.","(6) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(6) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.","(6) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.","(6) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.","(6) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.","(6) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment."]
["","","","","","(7) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(7) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.","(7) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(7) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(7) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(7) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(7) - 15°C-25°C: BUH only, no heat pump operation = during commissioning"]
["","","","","","(8) - For *RLQ* outdoor units >55°C BUH only, no heatpump operation","(8) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(8) - For *RLQ* outdoor units >55°C BUH only, no heatpump operation","(8) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models","(8) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models","(8) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models","(8) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models"]
["","","","","","","(9) - Lower if back-up heater is installed; In case of no back-up heater, then heat pump operation starts at 10°C","","(9) - For *RLQ* outdoor units >55°C BUH only, no heatpump operation","(9) - For *RLQ* outdoor units >55°C BUH only, no heatpump operation","(9) - For *RLQ* outdoor units >55°C BUH only, no heatpump operation","(9) - For *RLQ* outdoor units >55°C BUH only, no heatpump operation"]
["","","","","","","(10) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models","","(10) - For *RHQ* outdoor units >50°C BUH only, no heatpump operation","(10) - For *RHQ* outdoor units >50°C BUH only, no heatpump operation","(10) - For *RHQ* outdoor units >50°C BUH only, no heatpump operation","(10) - For *RHQ* outdoor units >50°C BUH only, no heatpump operation"]
["","","","","","","(11) - For *RLQ* outdoor units >55°C BUH only, no heatpump operation"]
["","","","","","","(12) - Unit performances refer to ideal running conditions that are reproducible in laboratory test environment in accordance to recognized industry standards (i.e. EN14511)"]
["","","","","","","(13) - For *RHQ* outdoor units >50°C BUH only, no heatpump operation"]
["","","","","","","(14) - Above mentioned power supply of the hydrobox is for the backup heater only. The switch box and the pump of the hydrobox are supplied via the outdoor unit."]
["","","","","","","(15) - Select diameter and type according to national and local regulations"]
["Casing","Colour","","","","White","","White","White","White","White","White"]
["","Material","","","","Precoated sheet metal","","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal"]
["Dimensions","Unit","","Height","mm","1732","","1732","1732","1732","1732","1732"]
["","","","Width","mm","600","","600","600","600","600","600"]
["","","","Depth","mm","728","","728","728","728","728","728"]
["Weight","Unit","","","kg","116","","127","126","117","128","118"]
["PED","Category","","","","Art3§3, See note 1","","Category I, See note 1","Art3§3, See note 1","Art3§3, See note 1","Art3§3, See note 1","Art3§3, See note 1"]
["Sound power level","Nom.","","","dBA","42.0 (6)","","42.0 (6)","42.0 (6)","42.0 (6)","44.0 (6)","44.0 (6)"]
["Sound pressure level","Nom.","","","dBA","28.0 (7)","","28.0 (7)","28.0 (7)","28.0 (7)","30.0 (7)","30.0 (7)"]
["Operation range","Heating","Water side","Min.","°C","15 (8)","","15 (8)","15 (8)","15 (8)","15 (8)","15 (8)"]
["","","","Max.","°C","55.0","","55.0","55.0 (10)","55.0 (10)","55.0 (10)","55.0 (10)"]
["Power supply","Name","","","","See note 14","","See note 14","See note 14","See note 14","See note 14","See note 14"]
["Electric heater","Power supply","","Name","","3V3","","9W","9W","3V3","9W","3V3"]
["","","","Phase","","1~","","Refer to installation manual or drawing 4D093592","Refer to installation manual or drawing 4D093592","1~","Refer to installation manual or drawing 4D093592","1~"]
["","","","Frequency","Hz","50","","50","50","50","50","50"]
["","","","Voltage","V","230","","","","230","","230"]
["Wiring connections","For connection with user interface","","Quantity","","2","","2","2","2","2","2"]
["","","","Remark","","0.75 mm² till 1.25 mm² (max length 500m)","","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)"]