{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":10,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-C / ERHQ-BW1"]
[]
[]
[]
[]
["","","","","EHVX16S18CA3V / ERHQ011BAW1","EHVX16S26CA9W / ERHQ011BAW1","EHVX16S18CA3V / ERHQ014BAW1","EHVX16S26CA9W / ERHQ014BAW1","EHVX16S18CA3V / ERHQ016BAW1","EHVX16S26CA9W / ERHQ016BAW1"]
["COP","","","","4.30 (3), 3.39 (4)","4.30 (3), 3.39 (4)","4.24 (3), 3.22 (4)","4.24 (3), 3.22 (4)","4.20 (3), 3.22 (4)","4.20 (3), 3.22 (4)"]
["Cooling capacity","Nom.","","kW","15.05 (2), 11.72 (1)","15.05 (2), 11.72 (1)","16.06 (2), 12.55 (1)","16.06 (2), 12.55 (1)","16.76 (2), 13.12 (1)","16.76 (2), 13.12 (1)"]
["EER","","","","3.32 (2), 2.72 (1)","3.32 (2), 2.72 (1)","2.96 (2), 2.47 (1)","2.96 (2), 2.47 (1)","2.72 (2), 2.29 (1)","2.72 (2), 2.29 (1)"]
["Heating capacity","Nom.","","kW","11.32 (3), 10.98 (4)","11.32 (3), 10.98 (4)","14.50 (3), 13.57 (4)","14.50 (3), 13.57 (4)","16.05 (3), 15.11 (4)","16.05 (3), 15.11 (4)"]
["Power input","Heating","Nom.","kW","2.63 (3), 3.24 (4)","2.63 (3), 3.24 (4)","3.42 (3), 4.21 (4)","3.42 (3), 4.21 (4)","3.82 (3), 4.69 (4)","3.82 (3), 4.69 (4)"]
["","Cooling","Nom.","kW","4.53 (2), 4.31 (1)","4.53 (2), 4.31 (1)","5.43 (2), 5.08 (1)","5.43 (2), 5.08 (1)","6.16 (2), 5.73 (1)","6.16 (2), 5.73 (1)"]
["Notes","","","","(1) - Tamb 35°C - LWE 7°C (DT=5°C)","(1) - Tamb 35°C - LWE 7°C (DT=5°C)","(1) - Tamb 35°C - LWE 7°C (DT=5°C)","(1) - Tamb 35°C - LWE 7°C (DT=5°C)","(1) - Tamb 35°C - LWE 7°C (DT=5°C)","(1) - Tamb 35°C - LWE 7°C (DT=5°C)"]
["","","","","(2) - Tamb 35°C - LWE 18°C (DT=5°C)","(2) - Tamb 35°C - LWE 18°C (DT=5°C)","(2) - Tamb 35°C - LWE 18°C (DT=5°C)","(2) - Tamb 35°C - LWE 18°C (DT=5°C)","(2) - Tamb 35°C - LWE 18°C (DT=5°C)","(2) - Tamb 35°C - LWE 18°C (DT=5°C)"]
["","","","","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)"]
["","","","","(4) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(4) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(4) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(4) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(4) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(4) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]