{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":16,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-C / ERLQ-CV3"]
[]
[]
[]
[]
["","","","","","EHVX04S18CA3V / ERLQ004CAV3","EHVX08S18CA3V / ERLQ006CAV3","EHVX08S26CA9W / ERLQ006CAV3","EHVX08S18CA3V / ERLQ008CAV3","EHVX08S26CA9W / ERLQ008CAV3","EHVX16S18CA3V / ERLQ011CAV3","EHVX16S26CA9W / ERLQ011CAV3","EHVX16S18CA3V / ERLQ014CAV3","EHVX16S26CA9W / ERLQ014CAV3","EHVX16S26CA9W / ERLQ016CAV3","EHVX16S18CA3V / ERLQ016CAV3"]
["COP","","","","","5.04 (1), 3.58 (2)","4.74 (1), 3.56 (2)","4.74 (1), 3.56 (2)","4.45 (1), 3.42 (2)","4.45 (1), 3.42 (2)","4.6 (1), 2.75 (3), 3.55 (2), 2.10 (4)","4.6 (1), 2.75 (3), 3.55 (2), 2.10 (4)","4.3 (1), 2.65 (3), 3.32 (2), 2.08 (4)","4.3 (1), 2.65 (3), 3.32 (2), 2.08 (4)","4.25 (1), 2.64 (3), 3.26 (2), 2.09 (4)","4.25, 2.64, 3.26, 2.09"]
["Cooling capacity","Nom.","","","kW","5.00 (1), 4.17 (2)","6.76 (1), 4.84 (2)","6.76 (1), 4.84 (2)","6.86 (1), 5.36 (2)","6.86 (1), 5.36 (2)","15.05 (1), 11.72 (2)","15.05 (1), 11.72 (2)","16.06 (1), 12.55 (2)","16.06 (1), 12.55 (2)","16.76 (1), 13.12 (2)"]
["","Min.","","","kW","2.00 (1), 2.00 (2)","2.50 (1), 2.50 (2)","2.50 (1), 2.50 (2)","2.50 (1), 2.50 (2)","2.50 (1), 2.50 (2)"]
["EER","","","","","3.37 (1), 2.32 (2)","3.45 (1), 2.34 (2)","3.45 (1), 2.34 (2)","3.42 (1), 2.29 (2)","3.42 (1), 2.29 (2)","3.32 (1), 2.72 (2)","3.32 (1), 2.72 (2)","2.96 (1), 2.47 (2)","2.96 (1), 2.47 (2)","2.72 (1), 2.29 (2)","2.72, 2.29"]
["Heating capacity","Nom.","","","kW","4.40 (1), 4.03 (2)","6.00 (1), 5.67 (2)","6.00 (1), 5.67 (2)","7.40 (1), 6.89 (2)","7.40 (1), 6.89 (2)","11.2 (1), 11.00 (2)","11.2 (1), 11.00 (2)","14.5 (1), 13.60 (2)","14.5 (1), 13.60 (2)","16 (1), 15.20 (2)"]
["","Min.","","","kW","1.80 (1), 1.80 (2)","1.80 (1), 1.80 (2)","1.80 (1), 1.80 (2)","1.80 (1), 1.80 (2)","1.80 (1), 1.80 (2)"]
["","Max.","","","kW","5.12 (1), 4.90 (2)","8.35 (1), 7.95 (2)","8.35 (1), 7.95 (2)","10.02 (1), 9.53 (2)","10.02 (1), 9.53 (2)","8.6 (3), 8.60 (4)","8.6 (3), 8.60 (4)","10.6 (3), 10.80 (4)","10.6 (3), 10.80 (4)","11.4 (3), 10.90 (4)"]
["Power input","Heating","","Max.","kW","","","","","","3.13 (3), 4.10 (4)","3.13 (3), 4.10 (4)","4.00 (3), 5.19 (4)","4.00 (3), 5.19 (4)","4.32 (3), 5.22 (4)"]
["","","","Nom.","kW","0.87 (1), 1.13 (2)","1.27 (1), 1.59 (2)","1.27 (1), 1.59 (2)","1.66 (1), 2.01 (2)","1.66 (1), 2.01 (2)","2.43 (1), 3.10 (2)","2.43 (1), 3.10 (2)","3.37 (1), 4.10 (2)","3.37 (1), 4.10 (2)","3.76 (1), 4.66 (2)"]
["","Cooling","","Nom.","kW","1.48 (1), 1.80 (2)","1.96 (1), 2.07 (2)","1.96 (1), 2.07 (2)","2.01 (1), 2.34 (2)","2.01 (1), 2.34 (2)","4.53 (1), 4.31 (2)","4.53 (1), 4.31 (2)","5.43 (1), 5.08 (2)","5.43 (1), 5.08 (2)","6.16 (1), 5.73 (2)"]
["Notes","","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["","","","","","(3) - Tamb 35°C - LWE 7°C (DT=5°C)","(3) - Tamb 35°C - LWE 7°C (DT=5°C)","(3) - Tamb 35°C - LWE 7°C (DT=5°C)","(3) - Tamb 35°C - LWE 7°C (DT=5°C)","(3) - Tamb 35°C - LWE 7°C (DT=5°C)","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C"]
["","","","","","(4) - Tamb 35°C - LWE 18°C (DT=5°C)","(4) - Tamb 35°C - LWE 18°C (DT=5°C)","(4) - Tamb 35°C - LWE 18°C (DT=5°C)","(4) - Tamb 35°C - LWE 18°C (DT=5°C)","(4) - Tamb 35°C - LWE 18°C (DT=5°C)","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C"]
["","","","","","(5) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(5) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(5) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(5) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(5) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","","","","","","(5) - Tamb 35°C - LWE 7°C (DT=5°C)"]
["","","","","","(6) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(6) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(6) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(6) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(6) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","","","","","","(6) - Tamb 35°C - LWE 18°C (DT=5°C)"]
["Heating capacity","Nom.","","","kW","","","","","","","","","","","16, 15.20"]
["","Max.","","","kW","","","","","","","","","","","11.4, 10.90"]
["Cooling capacity","Nom.","","","kW","","","","","","","","","","","16.76, 13.12"]
["Power input","Heating","","Nom.","kW","","","","","","","","","","","3.76, 4.66"]
["","","","Max.","kW","","","","","","","","","","","4.32, 5.22"]
["","Cooling","","Nom.","kW","","","","","","","","","","","6.16, 5.73"]
["Domestic hot water heating","General","","Declared load profile","","","","","","","","","","","","L"]
["","Average climate","","Water heating energy efficiency class","","","","","","","","","","","","A"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","","","","","","","","","","","3.20"]
["","","","Seasonal space heating eff. class","","","","","","","","","","","","A+"]
["","Average climate water outlet 35°C","General","SCOP","","","","","","","","","","","","3.99"]
["","","","Seasonal space heating eff. class","","","","","","","","","","","","A+"]
["Notes","","","","","","","","","","","","","","","(7) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)"]
["","","","","","","","","","","","","","","","(8) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]