{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":10,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-C"]
[]
[]
[]
[]
["","","","","","EHVX04S18CA3V","EHVX08S18CA3V","EHVX08S26CA9W","EHVX16S26CA9W","EHVX16S18CA3V"]
["Sound pressure level","Nom.","","","dBA","","28","","33"]
["Water side Heat exchanger","Water flow rate","Cooling","Max.","l/min","","34","","50"]
["","","Heating","Max.","l/min","","34","","50"]
["Sound power level","Nom.","","","dBA","","42 (2)","","47 (2)"]
["Dimensions","Unit","","Width","mm","","600","","600"]
["","","","Depth","mm","","728","","728"]
["","","","Height","mm","","1,732","","1,732"]
["Casing","Material","","","","","Precoated sheet metal","","Precoated sheet metal"]
["","Colour","","","","","White","","White"]
["Weight","Unit","","","kg","","117","","129"]
["PED","Category","","","","","Category I","","Art3§3"]
["Wiring connections","For connection with user interface","","Remark","","","0.75 mm² till 1.25 mm² (max length 500m)","","0.75 mm² till 1.25 mm² (max length 500m)"]
["","","","Quantity","","","2","","2"]
["Notes","","","","","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897"]
["","","","","","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)"]
["","","","","","(3) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(3) - The sound pressure level is measured via a microphone at a 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.","(3) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(3) - The sound pressure level is measured via a microphone at a 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.","(3) - 15°C-25°C: BUH only, no heat pump operation = during commissioning"]
["","","","","","(4) - Including piping + PHE + back-up heater; excluding expansion vessel","(4) - The sound pressure level mentioned is valid for pump medium speed - 0 ESP / medium speed - nominal flow / high speed - nominal flow","(4) - Including piping + PHE + back-up heater; excluding expansion vessel","(4) - The sound pressure level mentioned is valid for pump medium speed - 0 ESP / medium speed - nominal flow / high speed - nominal flow","(4) - Including piping + PHE + back-up heater; excluding expansion vessel"]
["","","","","","","(5) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","","(5) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(5) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models"]
["","","","","","","(6) - Including piping + PHE + back-up heater; excluding expansion vessel","","(6) - Including piping + PHE + back-up heater; excluding expansion vessel"]
["","","","","","","(7) - Water circuit piping connections diameter is connection after ball valves, Connection at unit is G1-1/4 FEMALE","","(7) - Water circuit piping connections diameter is connection after ball valves, Connection at unit is G1-1/4 FEMALE"]
["","","","","","","(8) - See separate drawing for operation range","","(8) - See separate drawing for operation range"]
["","","","","","","(9) - For *RLQ* outdoor units >55°C BUH only, no heatpump operation","","(9) - For *RLQ* outdoor units >55°C BUH only, no heatpump operation"]
["","","","","","","(10) - For *RHQ* outdoor units >50°C BUH only, no heatpump operation","","(10) - For *RHQ* outdoor units >50°C BUH only, no heatpump operation"]
["","","","","","","(11) - Minimum flow is mentioned for heat pump operation. To allow backup heater to operate safety a higher minimum flow is required. For *3V models 12 l/min","","(11) - Minimum flow is mentioned for heat pump operation. To allow backup heater to operate safety a higher minimum flow is required. For *3V models 12 l/min"]
["","","","","","","(12) - Minimum flow is mentioned for heat pump operation. To allow backup heater to operate safety a higher minimum flow is required. For *9W models 15 l/min","","(12) - Minimum flow is mentioned for heat pump operation. To allow backup heater to operate safety a higher minimum flow is required. For *9W models 15 l/min"]
["","","","","","","(13) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models","","(13) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models"]
["","","","","","","(14) - PED unit category: Art3§3: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","","(14) - PED unit category: Art3§3: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC"]
["","","","","","","(15) - For more details on current & voltage range, refer to the installation manual.","","(15) - For more details on current & voltage range, refer to the installation manual."]
["Casing","Colour","","","","White","","White","","White"]
["","Material","","","","Precoated sheet metal","","Precoated sheet metal","","Precoated sheet metal"]
["Dimensions","Unit","","Height","mm","1732","","1732","","1732"]
["","","","Width","mm","600","","600","","600"]
["","","","Depth","mm","728","","728","","728"]
["Weight","Unit","","","kg","115","","126","","121"]
["PED","Category","","","","Art3§3","","Category I","","Art3§3"]
["Water side Heat exchanger","Water flow rate","Heating","Max.","l/min","25","","34","","50"]
["","","Cooling","Max.","l/min","25","","34","","50"]
["Sound power level","Nom.","","","dBA","42 (2)","","42 (2)","","47 (2)"]
["Sound pressure level","Nom.","","","dBA","28","","28","","33"]
["Operation range","Heating","Water side","Min.","°C","15 (5)","","15 (5)","","15 (5)"]
["","","","Max.","°C","55 (5)","","55 (5)","","55 (5)"]
["","Cooling","Ambient","Min.","°CDB","10","","10","","10"]
["","","Water side","Min.","°C","5","","5","","5"]
["","","","Max.","°C","22","","22","","22"]
["Wiring connections","For connection with user interface","","Quantity","","2","","2","","2"]
["","","","Remark","","0.75 mm² till 1.25 mm² (max length 500m)","","0.75 mm² till 1.25 mm² (max length 500m)","","0.75 mm² till 1.25 mm² (max length 500m)"]