{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":8,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVZ-CB3V / ERHQ-BV3"]
[]
[]
[]
[]
["","","","","","EHVZ16S18CB3V / ERHQ011BAV3","EHVZ16S18CB3V / ERHQ014BAV3","EHVZ16S18CB3V / ERHQ016BAV3"]
["Heating capacity","Nom.","","","kW","11.2, 10.3","14.0, 13.1","16.0, 15.2"]
["Power input","Heating","","Nom.","kW","2.55, 3.17","3.26, 4.04","3.92, 4.75"]
["COP","","","","","4.39, 3.25","4.29, 3.24","4.08, 3.20"]
["Domestic hot water heating","General","","Declared load profile","","L","L","L"]
["","Average climate","","Water heating energy efficiency class","","A","A","A"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","2.86","2.82","2.92"]
["","","","Seasonal space heating eff. class","","A+","A+","A+"]
["","Average climate water outlet 35°C","General","SCOP","","2.99","3.23","3.29"]
["","","","Seasonal space heating eff. class","","A++","A+","A+"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Notes","","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["","","","","","","(3) - Capacity must be split up over the additional and main zone. Refer to ESP-data for more details on available head (kPa).","(3) - Capacity must be split up over the additional and main zone. Refer to ESP-data for more details on available head (kPa)."]