{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVZ-CB3V / ERLQ-CV3"]
[]
[]
[]
[]
["","","","","EHVZ08S18CB3V / ERLQ008CAV3"]
["Domestic hot water heating","General","Declared load profile","","L"]
["","Average climate","Water heating energy efficiency class","","A"]
["COP","","","","4.45 (1), 3.42 (2)"]
["Heating capacity","Nom.","","kW","7.40 (1), 6.89 (2)"]
["","Min.","","kW","1.80 (1)"]
["","Max.","","kW","10.0 (1), 9.53 (2)"]
["Power input","Heating","Nom.","kW","1.66 (1), 2.01 (2)"]
["Notes","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["","","","","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C"]
["","","","","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C"]
["","","","","(5) - Capacity must be split up over the additional and main zone. Refer to ESP-data for more details on available head (kPa)."]
["","","","","(6) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)"]
["","","","","(7) - DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]
["","","","","(8) - 15°C-25°C: BUH only, no heat pump operation = during commissioning"]