{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVZ-CB3V"]
[]
[]
[]
[]
["","","","","","EHVZ04S18CB3V","EHVZ08S18CB3V","EHVZ16S18CB3V"]
["Casing","Colour","","","","White","White","White"]
["","Material","","","","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal"]
["Dimensions","Unit","","Height","mm","1,732","1,732","1,732"]
["","","","Width","mm","600","600","600"]
["","","","Depth","mm","728","728","728"]
["Weight","Unit","","","kg","121","122","121"]
["PED","Category","","","","Art3§3, See note 1","Category I, See note 1","Art3§3, See note 1"]
["Sound power level","Nom.","","","dBA","42","42","44 (6)"]
["Sound pressure level","Nom.","","","dBA","28","28","30 (7)"]
["Operation range","Heating","Water side","Min.","°C","15","15","15 (8)"]
["","","","Max.","°C","55","55","55 (9)"]
["Power supply","Name","","","","See note 12","See note 12","See note 12"]
["Electric heater","Power supply","","Name","","3V3","3V3","3V3"]
["","","","Phase","","1~","1~","1~"]
["","","","Frequency","Hz","50","50","50"]
["","","","Voltage","V","230","230","230"]
["Wiring connections","For connection with user interface","","Quantity","","2","2","2"]
["","","","Remark","","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)"]
["Notes","","","","","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation)."]
["","","","","","(2) - Heatloss according to EN12897","(2) - Heatloss according to EN12897","(2) - Heatloss according to EN12897"]
["","","","","","(3) - Including piping + PHE + back-up heater; excluding expansion vessel","(3) - Including piping + PHE + back-up heater; excluding expansion vessel","(3) - Including piping + PHE + back-up heater; excluding expansion vessel"]
["","","","","","(4) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(4) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(4) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)"]
["","","","","","(5) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.","(5) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.","(5) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment."]
["","","","","","(6) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(6) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(6) - 15°C-25°C: BUH only, no heat pump operation = during commissioning"]
["","","","","","(7) - For *RLQ* outdoor units >55°C BUH only, no heatpump operation","(7) - For *RLQ* outdoor units >55°C BUH only, no heatpump operation","(7) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models"]
["","","","","","","","(8) - For *RLQ* outdoor units >55°C BUH only, no heatpump operation"]
["","","","","","","","(9) - For *RHQ* outdoor units >50°C BUH only, no heatpump operation"]