{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":11,"n_cols":22,"rows_kept":11,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHBH-BB / ERHQ-BW1"]
[]
[]
[]
[]
["","","","","EKHBH016BB3V3 / ERHQ011BAW1","EKHBH016BB6T1 / ERHQ011BAW1","EKHBH016BB6V3 / ERHQ011BAW1","EKHBH016BB6WN / ERHQ011BAW1","EKHBH016BB9T1 / ERHQ011BAW1","EKHBH016BB9WN / ERHQ011BAW1","EKHBH016BB3V3 / ERHQ014BAW1","EKHBH016BB6T1 / ERHQ014BAW1","EKHBH016BB6V3 / ERHQ014BAW1","EKHBH016BB6WN / ERHQ014BAW1","EKHBH016BB9T1 / ERHQ014BAW1","EKHBH016BB9WN / ERHQ014BAW1","EKHBH016BB3V3 / ERHQ016BAW1","EKHBH016BB6T1 / ERHQ016BAW1","EKHBH016BB6V3 / ERHQ016BAW1","EKHBH016BB6WN / ERHQ016BAW1","EKHBH016BB9T1 / ERHQ016BAW1","EKHBH016BB9WN / ERHQ016BAW1"]
["COP","","","","4.46 (1), 3.48 (2)","4.46 (1), 3.48 (2)","4.46 (1), 3.48 (2)","4.46 (1), 3.48 (2)","4.46 (1), 3.48 (2)","4.46 (1), 3.48 (2)","4.35 (1), 3.29 (2)","4.35 (1), 3.29 (2)","4.35 (1), 3.29 (2)","4.35 (1), 3.29 (2)","4.35 (1), 3.29 (2)","4.35 (1), 3.29 (2)","4.30 (1), 3.29 (2)","4.30 (1), 3.29 (2)","4.30 (1), 3.29 (2)","4.30 (1), 3.29 (2)","4.30 (1), 3.29 (2)","4.30 (1), 3.29 (2)"]
["Heating capacity","Nom.","","kW","11.32 (1), 10.98 (2)","11.32 (1), 10.98 (2)","11.32 (1), 10.98 (2)","11.32 (1), 10.98 (2)","11.32 (1), 10.98 (2)","11.32 (1), 10.98 (2)","14.50 (1), 13.57 (2)","14.50 (1), 13.57 (2)","14.50 (1), 13.57 (2)","14.50 (1), 13.57 (2)","14.50 (1), 13.57 (2)","14.50 (1), 13.57 (2)","16.05 (1), 15.11 (2)","16.05 (1), 15.11 (2)","16.05 (1), 15.11 (2)","16.05 (1), 15.11 (2)","16.05 (1), 15.11 (2)","16.05 (1), 15.11 (2)"]
["Power input","Heating","Nom.","kW","2.54 (1), 3.15 (2)","2.54 (1), 3.15 (2)","2.54 (1), 3.15 (2)","2.54 (1), 3.15 (2)","2.54 (1), 3.15 (2)","2.54 (1), 3.15 (2)","3.33 (1), 4.12 (2)","3.33 (1), 4.12 (2)","3.33 (1), 4.12 (2)","3.33 (1), 4.12 (2)","3.33 (1), 4.12 (2)","3.33 (1), 4.12 (2)","3.73 (1), 4.60 (2)","3.73 (1), 4.60 (2)","3.73 (1), 4.60 (2)","3.73 (1), 4.60 (2)","3.73 (1), 4.60 (2)","3.73 (1), 4.60 (2)"]
["Notes","","","","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]