{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":22,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHBX-B / ERLQ-BW1"]
[]
[]
[]
[]
["","","","","EKHBX016BA3V3 / ERLQ011BAW1","EKHBX016BA6T1 / ERLQ011BAW1","EKHBX016BA6V3 / ERLQ011BAW1","EKHBX016BA6WN / ERLQ011BAW1","EKHBX016BA9T1 / ERLQ011BAW1","EKHBX016BA9WN / ERLQ011BAW1","EKHBX016BA3V3 / ERLQ014BAW1","EKHBX016BA6T1 / ERLQ014BAW1","EKHBX016BA6V3 / ERLQ014BAW1","EKHBX016BA6WN / ERLQ014BAW1","EKHBX016BA9T1 / ERLQ014BAW1","EKHBX016BA9WN / ERLQ014BAW1","EKHBX016BA3V3 / ERLQ016BAW1","EKHBX016BA6T1 / ERLQ016BAW1","EKHBX016BA6V3 / ERLQ016BAW1","EKHBX016BA6WN / ERLQ016BAW1","EKHBX016BA9T1 / ERLQ016BAW1","EKHBX016BA9WN / ERLQ016BAW1"]
["COP","","","","4.46 (1), 3.48 (2)","4.46 (1), 3.48 (2)","4.46 (1), 3.48 (2)","4.46 (1), 3.48 (2)","4.46 (1), 3.48 (2)","4.46 (1), 3.48 (2)","4.35 (1), 3.29 (2)","4.35 (1), 3.29 (2)","4.35 (1), 3.29 (2)","4.35 (1), 3.29 (2)","4.35 (1), 3.29 (2)","4.35 (1), 3.29 (2)","4.30 (1), 3.29 (2)","4.30 (1), 3.29 (2)","4.30 (1), 3.29 (2)","4.30 (1), 3.29 (2)","4.30 (1), 3.29 (2)","4.30 (1), 3.29 (2)"]
["Cooling capacity","Nom.","","kW","15.05 (1), 11.72 (2)","15.05 (1), 11.72 (2)","15.05 (1), 11.72 (2)","15.05 (1), 11.72 (2)","15.05 (1), 11.72 (2)","15.05 (1), 11.72 (2)","16.06 (1), 12.55 (2)","16.06 (1), 12.55 (2)","16.06 (1), 12.55 (2)","16.06 (1), 12.55 (2)","16.06 (1), 12.55 (2)","16.06 (1), 12.55 (2)","16.76 (1), 13.12 (2)","16.76 (1), 13.12 (2)","16.76 (1), 13.12 (2)","16.76 (1), 13.12 (2)","16.76 (1), 13.12 (2)","16.76 (1), 13.12 (2)"]
["EER","","","","3.39 (1), 2.78 (2)","3.39 (1), 2.78 (2)","3.39 (1), 2.78 (2)","3.39 (1), 2.78 (2)","3.39 (1), 2.78 (2)","3.39 (1), 2.78 (2)","3.01 (1), 2.51 (2)","3.01 (1), 2.51 (2)","3.01 (1), 2.51 (2)","3.01 (1), 2.51 (2)","3.01 (1), 2.51 (2)","3.01 (1), 2.51 (2)","2.76 (1), 2.32 (2)","2.76 (1), 2.32 (2)","2.76 (1), 2.32 (2)","2.76 (1), 2.32 (2)","2.76 (1), 2.32 (2)","2.76 (1), 2.32 (2)"]
["Heating capacity","Nom.","","kW","11.32 (1), 10.98 (2)","11.32 (1), 10.98 (2)","11.32 (1), 10.98 (2)","11.32 (1), 10.98 (2)","11.32 (1), 10.98 (2)","11.32 (1), 10.98 (2)","14.50 (1), 13.57 (2)","14.50 (1), 13.57 (2)","14.50 (1), 13.57 (2)","14.50 (1), 13.57 (2)","14.50 (1), 13.57 (2)","14.50 (1), 13.57 (2)","16.05 (1), 15.11 (2)","16.05 (1), 15.11 (2)","16.05 (1), 15.11 (2)","16.05 (1), 15.11 (2)","16.05 (1), 15.11 (2)","16.05 (1), 15.11 (2)"]
["Power input","Heating","Nom.","kW","2.54 (1), 3.15 (2)","2.54 (1), 3.15 (2)","2.54 (1), 3.15 (2)","2.54 (1), 3.15 (2)","2.54 (1), 3.15 (2)","2.54 (1), 3.15 (2)","3.33 (1), 4.12 (2)","3.33 (1), 4.12 (2)","3.33 (1), 4.12 (2)","3.33 (1), 4.12 (2)","3.33 (1), 4.12 (2)","3.33 (1), 4.12 (2)","3.73 (1), 4.60 (2)","3.73 (1), 4.60 (2)","3.73 (1), 4.60 (2)","3.73 (1), 4.60 (2)","3.73 (1), 4.60 (2)","3.73 (1), 4.60 (2)"]
["","Cooling","Nom.","kW","4.44 (1), 4.22 (2)","4.44 (1), 4.22 (2)","4.44 (1), 4.22 (2)","4.44 (1), 4.22 (2)","4.44 (1), 4.22 (2)","4.44 (1), 4.22 (2)","5.33 (1), 5.00 (2)","5.33 (1), 5.00 (2)","5.33 (1), 5.00 (2)","5.33 (1), 5.00 (2)","5.33 (1), 5.00 (2)","5.33 (1), 5.00 (2)","6.06 (1), 5.65 (2)","6.06 (1), 5.65 (2)","6.06 (1), 5.65 (2)","6.06 (1), 5.65 (2)","6.06 (1), 5.65 (2)","6.06 (1), 5.65 (2)"]
["Notes","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]