{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":6,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHBXE-B"]
[]
[]
[]
[]
["","","","","","EKHBXE008BA3V3"]
["Sound pressure level","Medium speed","","0 ESP","dBA","28 (10)"]
["Operation range","Cooling","Water side","Max.","°C","22"]
["","","","Min.","°C","5"]
["","Heating","Water side","Max.","°C","50 (12)"]
["","","","Min.","°C","15 (12)"]
["Sound power level","Medium speed","","0 ESP","dBA","42 (15)"]
["Dimensions","Unit","","Width","mm","502"]
["","","","Depth","mm","361"]
["","","","Height","mm","922"]
["Casing","Material","","","","Epoxy polyester painted galvanised steel"]
["","Colour","","","","RAL9010"]
["Weight","Unit","","","kg","46"]
["Electric heater","Current back-up heater","","Running current","A","13"]
["","Power supply","","Frequency","Hz","50"]
["","","","Voltage","V","230"]
["","","","Phase","","1~"]
["Notes","","","","","(1) - In combination with ERHQ006BAV3"]
["","","","","","(2) - In combination with ERLQ006BAV3"]
["","","","","","(3) - In combination with ERHQ007BAV3"]
["","","","","","(4) - In combination with ERLQ007BAV3"]
["","","","","","(5) - In combination with ERHQ008BAV3"]
["","","","","","(6) - In combination with ERLQ008BAV3"]
["","","","","","(7) - With option kit EKHBDP installed: Height = 936mm"]
["","","","","","(8) - Water flow rate cooling: Tamb 35°C - LWE 7°C (Dt=5°C)"]
["","","","","","(9) - Water flow rate heating: DB/WB 7°C/6°C - LWC 35°C (Dt=5°C)"]
["","","","","","(10) - The sound pressure level is measured via a microphone at a 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment."]
["","","","","","(11) - The sound pressure level mentioned is valid for pump medium speed - 0 ESP / medium speed - nominal flow / high speed - nominal flow"]
["","","","","","(12) - 15°C-25°C: BUH only, no heat pump operation = during commissioning"]
["","","","","","(13) - Including piping + PHE + back-up heater; excluding expansion vessel"]
["","","","","","(14) - Water circuit piping connections: value mentioned is connection after ball valves. Connection at unit is G1 1/2 female."]
["","","","","","(15) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), medium pump speed"]
["","","","","","(16) - Operation range EKHB(H/X)E008BA3V3: -15°C~25°C"]
["","","","","","(17) - Above mentioned power supply of the hydrobox is for the backup heater only. The switch box and the pump of the hydrobox are supplied via the outdoor unit. The optional domestic hot water tank has a separate power supply."]
["","","","","","(18) - Optional electric heater has 2 capacity steps except for the 3V3 model which has only 1 capacity step."]
["","","","","","(19) - In accordance with EN/IEC 61000-3-11, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply with Zsys (system impedance) ≤ Zmax"]
["","","","","","(20) - Equipment complying with EN/IEC 61000-3-12: European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current > 16A and ≤ 75A per phase"]
["","","","","","(21) - For EKHB*E008AA3V3 units: In case the \"restricted power supply\" mode is enabled, the booster heater and backup heater cannot work together. Current for booster heater is 13A."]
["","","","","","(22) - EN/IEC 61000-3-11: European/international technical standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated ≤ 75A"]