{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":13,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHVX-BB / ERLQ-CW1"]
[]
[]
[]
[]
["","","","","EKHVX016BB6V3 / ERLQ011CAW1","EKHVX016BB6WN / ERLQ011CAW1","EKHVX016BB9WN / ERLQ011CAW1","EKHVX016BB6V3 / ERLQ014CAW1","EKHVX016BB6WN / ERLQ014CAW1","EKHVX016BB9WN / ERLQ014CAW1","EKHVX016BB6V3 / ERLQ016CAW1","EKHVX016BB6WN / ERLQ016CAW1","EKHVX016BB9WN / ERLQ016CAW1"]
["COP","","","","4.66 (1), 3.48 (2), 2.57 (3), 2.01 (4)","4.66 (1), 3.48 (2), 2.57 (3), 2.01 (4)","4.66 (1), 3.48 (2), 2.57 (3), 2.01 (4)","4.46 (1), 3.29 (2), 2.40 (3), 1.97 (4)","4.46 (1), 3.29 (2), 2.40 (3), 1.97 (4)","4.46 (1), 3.29 (2), 2.40 (3), 1.97 (4)","4.30 (1), 3.29 (2), 2.28 (3), 1.82 (4)","4.30 (1), 3.29 (2), 2.28 (3), 1.82 (4)","4.30 (1), 3.29 (2), 2.28 (3), 1.82 (4)"]
["Cooling capacity","Nom.","","kW","15.05 (1), 11.72 (2)","15.05 (1), 11.72 (2)","15.05 (1), 11.72 (2)","16.06 (1), 12.55 (2)","16.06 (1), 12.55 (2)","16.06 (1), 12.55 (2)","16.76 (1), 13.12 (2)","16.76 (1), 13.12 (2)","16.76 (1), 13.12 (2)"]
["EER","","","","3.39 (1), 2.78 (2)","3.39 (1), 2.78 (2)","3.39 (1), 2.78 (2)","3.01 (1), 2.51 (2)","3.01 (1), 2.51 (2)","3.01 (1), 2.51 (2)","2.76 (1), 2.32 (2)","2.76 (1), 2.32 (2)","2.76 (1), 2.32 (2)"]
["Heating capacity","Nom.","","kW","11.20 (1), 10.98 (2)","11.20 (1), 10.98 (2)","11.20 (1), 10.98 (2)","14.00 (1), 13.57 (2)","14.00 (1), 13.57 (2)","14.00 (1), 13.57 (2)","16.00 (1), 15.20 (2)","16.00 (1), 15.20 (2)","16.00 (1), 15.20 (2)"]
["","Max.","","kW","8.81 (3), 8.16 (4)","8.81 (3), 8.16 (4)","8.81 (3), 8.16 (4)","11.65 (3), 10.96 (4)","11.65 (3), 10.96 (4)","11.65 (3), 10.96 (4)","12.30 (3), 11.35 (4)","12.30 (3), 11.35 (4)","12.30 (3), 11.35 (4)"]
["Power input","Heating","Max.","kW","3.43 (3), 4.05 (4)","3.43 (3), 4.05 (4)","3.43 (3), 4.05 (4)","4.86 (3), 5.57 (4)","4.86 (3), 5.57 (4)","4.86 (3), 5.57 (4)","5.40 (3), 6.25 (4)","5.40 (3), 6.25 (4)","5.40 (3), 6.25 (4)"]
["","","Nom.","kW","2.41 (1), 3.15 (2)","2.41 (1), 3.15 (2)","2.41 (1), 3.15 (2)","3.14 (1), 4.12 (2)","3.14 (1), 4.12 (2)","3.14 (1), 4.12 (2)","3.72 (1), 4.60 (2)","3.72 (1), 4.60 (2)","3.72 (1), 4.60 (2)"]
["","Cooling","Nom.","kW","4.44 (1), 4.22 (2)","4.44 (1), 4.22 (2)","4.44 (1), 4.22 (2)","5.33 (1), 5.00 (2)","5.33 (1), 5.00 (2)","5.33 (1), 5.00 (2)","6.06 (1), 5.65 (2)","6.06 (1), 5.65 (2)","6.06 (1), 5.65 (2)"]
["Notes","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["","","","","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C","(3) - Condition 3: heating Ta DB -7°C (RH85%) - LWC 35°C"]
["","","","","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C","(4) - Condition 4: heating Ta DB -7°C (RH85%) - LWC 45°C"]