{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERHQ-BW1"]
[]
[]
[]
[]
["","","","","","ERHQ011BAW1","ERHQ014BAW1","ERHQ016BAW1"]
["Sound pressure level","Heating","","Nom.","dBA","51 (5)","51 (5)","52 (5)"]
["","Cooling","","Nom.","dBA","50 (6)","52 (6)","54 (6)"]
["Sound power level","Heating","","Nom.","dBA","64 (3)","64 (3)","66 (3)"]
["","Cooling","","Nom.","dBA","64 (4)","66 (4)","69 (4)"]
["Refrigerant","Charge","","","TCO2Eq","6.3","6.3","6.3"]
["","GWP","","","","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","3.0","3.0","3.0"]
["","Type","","","","R-410A","R-410A","R-410A"]
["Dimensions","Unit","","Width","mm","900","900","900"]
["","","","Depth","mm","320","320","320"]
["","","","Height","mm","1,345","1,345","1,345"]
["Weight","Unit","","","kg","108","108","108"]
["Operation range","Cooling","","Max.","°CDB","46.0","","46.0"]
["","","","Min.","°CDB","10.0","","10.0"]
["","Domestic hot water","","Min.","°CDB","-20 (2)","","-20 (2)"]
["","","","Max.","°CDB","35 (2)","","35 (2)"]
["Piping connections","Heat insulation","","","","Both liquid and gas pipes","Both liquid and gas pipes","Both liquid and gas pipes"]
["","Liquid","","OD","mm","9.52","9.52","9.52"]
["","Gas","","OD","mm","15.90","15.90","15.90"]
["","Drain","","OD","mm","26","26","26"]
["","Level difference","IU - OU","Max.","m","30.0","30.0","30.0"]
["Power supply","Phase","","","","3N~","3N~","3N~"]
["","Name","","","","W1","W1","W1"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","400","400","400"]
["Current","Recommended fuses","","","A","20","20","20"]
["Notes","","","","","(1) - Operation range heating (outdoor unit): range increase by support back-up heater. See separate drawing for operation range.","(1) - Operation range heating (outdoor unit): range increase by support back-up heater. See separate drawing for operation range.","(1) - Operation range heating (outdoor unit): range increase by support back-up heater. See separate drawing for operation range."]
["","","","","","(2) - Operation range domestic hot water (outdoor unit): range increase by support booster heater or backup heater. See separate drawing for operation range.","(2) - Operation range domestic hot water (outdoor unit): range increase by support booster heater or backup heater. See separate drawing for operation range.","(2) - Operation range domestic hot water (outdoor unit): range increase by support booster heater or backup heater. See separate drawing for operation range."]
["","","","","","(3) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(4) - Condition: Ta 35°C - LWE 7°C ( DT = 5°C)","(4) - Condition: Ta 35°C - LWE 7°C ( DT = 5°C)","(4) - Condition: Ta 35°C - LWE 7°C ( DT = 5°C)"]
["","","","","","(5) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta DB/WB 7°C/6°C - LWC 3","(5) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C).","(5) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta DB/WB 7°C/6°C - LWC 3"]
["","","","","","(6) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta 35°C - LWE 7°C ( DT =","(6) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta 35°C - LWE 7°C ( DT = 5°C).","(6) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information. Condition: Ta 35°C - LWE 7°C ( DT ="]
["","","","","","(7) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(7) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(7) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information."]
["","","","","","(8) - Down to 3m with recharging of the outdoor unit. Please refer to the installation manual of the outdoor unit.","(8) - Down to 3m with recharging of the outdoor unit. Please refer to the installation manual of the outdoor unit.","(8) - Down to 3m with recharging of the outdoor unit. Please refer to the installation manual of the outdoor unit."]
["","","","","","(9) - Contains fluorinated greenhouse gases","(9) - Contains fluorinated greenhouse gases","(9) - Contains fluorinated greenhouse gases"]