{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":11,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERLQ-BV3"]
[]
[]
[]
[]
["","","","","","ERLQ006BAV3","ERLQ007BAV3","ERLQ008BAV3","ERLQ011BAV3","ERLQ014BAV3","ERLQ016BAV3"]
["Sound pressure level","Heating","","Nom.","dBA","48","48","49","49","51","53"]
["","Cooling","","Nom.","dBA","48","48","50","50","52","54"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","3.5","3.5","3.5","7.7","7.7","7.7"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","1.7","1.7","1.7","3.7","3.7","3.7"]
["","Type","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Piping connections","Heat insulation","","","","","","","Both liquid and gas pipes","Both liquid and gas pipes","Both liquid and gas pipes"]
["","Liquid","","OD","mm","6.35","6.35","6.35","9.52","9.52","9.52"]
["","Gas","","OD","mm","15.9","15.9","15.9","15.9","15.9","15.9"]
["","Drain","","OD","mm","18","18","18","26","26","26"]
["","Level difference","IU - IU","Max.","m","20","20","20"]
["","","IU - OU","Max.","m","","","","30","30","30"]
["Sound power level","Heating","","Nom.","dBA","61","61","62","64","64","66"]
["","Cooling","","Nom.","dBA","63","63","63","64","66","69"]
["Dimensions","Unit","","Width","mm","825","825","825","900","900","900"]
["","","","Depth","mm","300","300","300","320","320","320"]
["","","","Height","mm","735","735","735","1,170","1,170","1,170"]
["Weight","Unit","","","kg","57","57","57","103","103","103"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Name","","","","V3","V3","V3","V3","V3","V3"]
["","Frequency","","","Hz","50","50","50","50","50","50"]
["","Voltage","","","V","230","230","230","230","230","230"]
["Current","Recommended fuses","","","A","20","20","20","32","32","32"]
["Notes","","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - Down to 3m with recharging of the outdoor unit. Please refer to the installation manual of the outdoor unit.","(1) - Down to 3m with recharging of the outdoor unit. Please refer to the installation manual of the outdoor unit.","(1) - Down to 3m with recharging of the outdoor unit. Please refer to the installation manual of the outdoor unit."]
["","","","","","(2) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(2) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(2) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(2) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(2) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(2) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information."]
["","","","","","(3) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","(3) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","(3) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","(3) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","(3) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase","(3) - Minimum Ssc value: Equipment complying with EN/IEC 61000-3-12: European/International Technical Standard setting the limits for harmonic currents produced by equipment connected to public low-voltage systems with input current >16A and ≤ 75A per phase"]
["","","","","","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases"]
["Standard Accessories","Tie-wraps","","","","","","","2","2","2"]