{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":11,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERLQ-CV3"]
[]
[]
[]
[]
["","","","","","ERLQ004CAV3","ERLQ006CAV3","ERLQ008CAV3","ERLQ011CAV3","ERLQ014CAV3","ERLQ016CAV3"]
["Sound pressure level","Heating","","Nom.","dBA","","48 (3)","49 (3)","51 (5)","51 (5)","52 (5)"]
["","Cooling","","Nom.","dBA","","49 (3)","50 (3)","50 (5)","52 (5)","54 (5)"]
["Sound power level","Heating","","Nom.","dBA","","61","62","64 (3)","64 (3)","66 (3)"]
["","Cooling","","Nom.","dBA","","63","63","64 (4)","66 (4)","69 (4)"]
["Refrigerant","Charge","","","TCO2Eq","","3.3","3.3"]
["","GWP","","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","","1.6","1.6","3.4","3.4","3.4"]
["","Type","","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Dimensions","Unit","","Width","mm","","832","832","900","900","900"]
["","","","Depth","mm","","307","307","320","320","320"]
["","","","Height","mm","","735","735","1,345","1,345","1,345"]
["Weight","Unit","","","kg","","56","56","113","113","113"]
["Operation range","Cooling","","Max.","°CDB","","43.0","43.0","46.0","46.0","46.0"]
["","","","Min.","°CDB","","10.0","10.0","10.0","10.0","10.0"]
["","Domestic hot water","","Min.","°CDB","","-25 (2)","-25 (2)","-20 (2)","-20 (2)","-20 (2)"]
["","","","Max.","°CDB","","35 (2)","35 (2)","35 (2)","35 (2)","35 (2)"]
["Piping connections","Heat insulation","","","","","Both liquid and gas pipes","Both liquid and gas pipes","Both liquid and gas pipes","Both liquid and gas pipes","Both liquid and gas pipes"]
["","Liquid","","OD","mm","","6.35","6.35","9.52","9.52","9.52"]
["","Gas","","OD","mm","","15.90","15.90","15.90","15.90","15.90"]
["","Drain","","OD","mm","","1x ø15 + 1x ø20","1x ø15 + 1x ø20","26","26","26"]
["","Level difference","IU - OU","Max.","m","","20.0","20.0","30.0","30.0","30.0"]
["Power supply","Phase","","","","","1~","1~","1~","1~","1~"]
["","Name","","","","","V3","V3","V3","V3","V3"]
["","Frequency","","","Hz","","50","50","50","50","50"]
["","Voltage","","","V","","230","230","230","230","230"]
["Current","Recommended fuses","","","A","","16","20","40","40","40"]
["Notes","","","","","(1) - Operation range heating (outdoor unit): range increase by support back-up heater. See separate drawing for operation range.","(1) - Operation range heating (outdoor unit): range increase by support back-up heater. See separate drawing for operation range.","(1) - Operation range heating (outdoor unit): range increase by support back-up heater. See separate drawing for operation range.","(1) - Operation range heating (outdoor unit): range increase by support back-up heater. See separate drawing for operation range.","(1) - Operation range heating (outdoor unit): range increase by support back-up heater. See separate drawing for operation range.","(1) - Operation range heating (outdoor unit): range increase by support back-up heater. See separate drawing for operation range."]
["","","","","","(2) - Operation range domestic hot water (outdoor unit): range increase by support booster heater or backup heater. See separate drawing for operation range.","(2) - Operation range domestic hot water (outdoor unit): range increase by support booster heater or backup heater. See separate drawing for operation range.","(2) - Operation range domestic hot water (outdoor unit): range increase by support booster heater or backup heater. See separate drawing for operation range.","(2) - Operation range domestic hot water (outdoor unit): range increase by support booster heater or backup heater. See separate drawing for operation range.","(2) - Operation range domestic hot water (outdoor unit): range increase by support booster heater or backup heater. See separate drawing for operation range.","(2) - Operation range domestic hot water (outdoor unit): range increase by support booster heater or backup heater. See separate drawing for operation range."]
["","","","","","(3) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(3) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(3) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(3) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(4) - Daikin Altherma inverter controlled compressor starting current always <= max. running current","(4) - Daikin Altherma inverter controlled compressor starting current always <= max. running current","(4) - Daikin Altherma inverter controlled compressor starting current always <= max. running current","(4) - Condition: Ta 35°C - LWE 7°C ( DT = 5°C)","(4) - Condition: Ta 35°C - LWE 7°C ( DT = 5°C)","(4) - Condition: Ta 35°C - LWE 7°C ( DT = 5°C)"]
["","","","","","(5) - Contains fluorinated greenhouse gases","(5) - Contains fluorinated greenhouse gases","(5) - Contains fluorinated greenhouse gases","(5) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(5) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(5) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information."]
["Dimensions","Unit","","Height","mm","735"]
["","","","Width","mm","832"]
["","","","Depth","mm","307"]
["Weight","Unit","","","kg","54"]
["Operation range","Cooling","","Min.","°CDB","10"]
["","","","Max.","°CDB","43"]
["","Domestic hot water","","Min.","°CDB","-25 (2)"]
["","","","Max.","°CDB","35 (2)"]
["Sound power level","Heating","","Nom.","dBA","61"]
["","Cooling","","Nom.","dBA","63"]
["Sound pressure level","Heating","","Nom.","dBA","48 (3)"]
["","Cooling","","Nom.","dBA","48 (3)"]
["Refrigerant","Type","","","","R-410A"]
["","GWP","","","","2,087.5"]
["","Charge","","","tCO2Eq","3.1"]
["","Charge","","","kg","1.5"]
["Piping connections","Liquid","","OD","mm","6.35"]
["","Gas","","OD","mm","15.9"]
["","Drain","","OD","mm","1x ø15 + 1x ø20"]
["","Level difference","IU - OU","Max.","m","20.0"]
["","Heat insulation","","","","Both liquid and gas pipes"]
["Power supply","Name","","","","V3"]
["","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","230"]
["Current","Recommended fuses","","","A","16"]
["Notes","","","","","","","","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases"]