{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-B"]
[]
[]
[]
[]
["","","","","FAQ71BVV1B","FAQ100BVV1B"]
["Sound pressure level","Heating","High","dBA","43.0","45.0"]
["","","Low","dBA","37.0","41.0"]
["","Cooling","Low","dBA","37.0","41.0"]
["","","High","dBA","43.0","45.0"]
["Standard Accessories","Installation and operation manual","","","1","1"]
["","Paper pattern for installation","","","Paper pattern for installation","Paper pattern for installation"]
["","Insulation tape","","","Insulation tape","Insulation tape"]
["","Insulation for fitting","","","","Insulation for fitting"]
["","Installation panel","","","Installation panel","Installation panel"]
["","Screws","","","Screws","Screws"]
["Piping connections","Liquid","OD","mm","9.52","9.52"]
["","Gas","OD","mm","15.9","15.9"]
["","Drain","","","VP13 (I.D. 13/O.D. 18)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Cooling","","dBA","59.0","61.0"]
["","Heating","","dBA","59.0","61.0"]
["Dimensions","Unit","Width","mm","1,050","1,570"]
["","","Depth","mm","230","200"]
["","","Height","mm","290","360"]
["Casing","Material","","","Resin","Resin"]
["","Colour","","","White","White"]
["Weight","Unit","","kg","13.0","26.0"]
["Power supply","Phase","","","1~","1~"]
["","Frequency","","Hz","50","50"]
["","Voltage","","V","220-240","220-240"]
["Notes","","","","(1) - The sound pressure level is measured via a microphone at 1m distance of the unit.","(1) - The sound pressure level is measured via a microphone at 1m distance of the unit."]
["","","","","(2) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(2) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings."]
["","","","","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates."]