{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / ARXM-R"]
[]
[]
[]
[]
["","","","","FBA71A2VEB9 / ARXM71R2V1B","FBA71A2VEB9 / ARXM71R5V1B"]
["Cooling capacity","Max.","","kW","6.98","6.98"]
["","Nom.","","kW","6.80","6.80"]
["Space cooling","SEER","","","5.57","5.57"]
["","Annual energy consumption","","kWh/a","427","427"]
["","Capacity","Pdesign","kW","6.80","6.80"]
["","Energy efficiency class","","","A","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.50","4.50"]
["","SCOP/A","","","3.81","3.81"]
["","Energy efficiency class","","","A","A"]
["","Annual energy consumption","","kWh/a","1,652","1,652"]
["Nominal efficiency","Annual energy consumption","","kWh","944","944"]
["","EER","","","3.60","3.60"]
["","COP","","","3.67","3.67"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Heating capacity","Nom.","","kW","7.50","7.50"]
["","Max.","","kW","7.66","7.66"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]