{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":44,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RZAG-NY1"]
[]
[]
[]
[]
["","","","","FBA100A2VEB / RZAG71N2Y1B","FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / RZAG71N2Y1B","FBA50A2VEB9 / FBA50A2VEB9 / RZAG71N2Y1B","FBA100A2VEB / RZAG71N7Y1B","FBA35A2VEB9 / FBA35A2VEB9 / RZAG71N7Y1B","FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / RZAG71N7Y1B","FBA71A2VEB9 / RZAG71N7Y1B","FBA50A2VEB9 / FBA50A2VEB9 / RZAG71N7Y1B","FBA71A2VEB9 / RZAG71N2Y1B","FBA35A2VEB9 / FBA35A2VEB9 / RZAG71N2Y1B","FBA140A2VEB / RZAG100N2Y1B","FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / RZAG100N2Y1B","FBA50A2VEB9 / FBA50A2VEB9 / FBA50A2VEB9 / RZAG100N2Y1B","FBA71A2VEB9 / FBA71A2VEB9 / RZAG100N2Y1B","FBA100A2VEB / RZAG100N7Y1B","FBA140A2VEB / RZAG100N7Y1B","FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / RZAG100N7Y1B","FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / RZAG100N7Y1B","FBA50A2VEB9 / FBA50A2VEB9 / RZAG100N7Y1B","FBA71A2VEB9 / FBA71A2VEB9 / RZAG100N7Y1B","FBA50A2VEB9 / FBA50A2VEB9 / FBA50A2VEB9 / RZAG100N7Y1B","FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / RZAG100N2Y1B","FBA100A2VEB / RZAG100N2Y1B","FBA50A2VEB9 / FBA50A2VEB9 / RZAG100N2Y1B","FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / RZAG125N7Y1B","FBA50A2VEB9 / FBA50A2VEB9 / FBA50A2VEB9 / RZAG125N2Y1B","FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / RZAG125N2Y1B","FBA125A2VEB / RZAG125N2Y1B","FBA60A2VEB9 / FBA60A2VEB9 / RZAG125N2Y1B","FBA50A2VEB9 / FBA50A2VEB9 / FBA50A2VEB9 / RZAG125N7Y1B","FBA60A2VEB9 / FBA60A2VEB9 / RZAG125N7Y1B","FBA125A2VEB / RZAG125N7Y1B","FBA140A2VEB / RZAG140N7Y1B","FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / RZAG140N7Y1B","FBA71A2VEB9 / FBA71A2VEB9 / RZAG140N2Y1B","FBA140A2VEB / RZAG140N2Y1B","FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / RZAG140N2Y1B","FBA50A2VEB9 / FBA50A2VEB9 / FBA50A2VEB9 / RZAG140N2Y1B","FBA50A2VEB9 / FBA50A2VEB9 / FBA50A2VEB9 / RZAG140N7Y1B","FBA71A2VEB9 / FBA71A2VEB9 / RZAG140N7Y1B"]
["Cooling capacity","Nom.","","kW","6.80 (1)","6.80 (1)","6.80 (1)","6.80 (1)","6.80 (1)","6.80 (1)","6.80 (1)","6.80 (1)","6.80 (1)","6.80 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)","12.1 (1)","12.1 (1)","12.1 (1)","12.1 (1)","12.1 (1)","","","","13.4 (1)","13.4 (1)","13.4 (1)","13.4 (1)","13.4 (1)","13.4 (1)"]
["Space cooling","SEER","","","5.81","5.08","5.45","5.81","6.46","5.08","6.50","5.45","6.50","6.46","6.39","5.81","6.54","7.88","6.47","6.39","6.65","5.81","6.52","7.88","6.54","6.65","6.47","6.52","11.2","9.74","11.2","6.56","8.80","","","","6.42","11.4","8.80","6.42","11.4","8.95"]
["","ηs,c","","%","","","","","","","","","","","","","","","","","","","","","","","","","445","","","","","","","","254","452"]
["","Annual energy consumption","","kWh/a","410","469","437","410","368","469","366","437","366","368","520","572","508","422","514","520","500","572","510","422","508","500","514","510","649","745","649","1,107","825","","","","1,252","707","914","1,252","707","898"]
["","Capacity","Pdesign","kW","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","9.50","9.50","9.50","9.50","9.50","9.50","9.50","9.50","9.50","9.50","9.50","9.50","9.50","9.50","12.1","12.1","12.1","12.1","12.1","","","","13.4","13.4","13.4","13.4","13.4","13.4"]
["","Energy efficiency class","","","A+","B","A","A+","A++","B","A++","A","A++","A++","A++","A+","A++","A++","A++","A++","A++","A+","A++","A++","A++","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.70","4.70","4.70","4.70","4.70","4.70","4.70","4.70","4.70","4.70","7.80","7.80","7.80","7.80","7.80","7.80","7.80","7.80","7.80","7.80","7.80","7.80","7.80","7.80","9.52","9.52","9.52","9.52","9.52","","","","9.52","9.52","9.52","9.52","9.52","9.52"]
["","SCOP/A","","","4.06","3.80","3.88","4.06","4.10","3.80","4.20","3.88","4.20","4.10","4.20","3.92","4.06","4.43","4.36","4.20","4.14","3.92","4.12","4.43","4.06","4.14","4.36","4.12","5.85","4.75","5.85","4.37","4.31","","","","4.34","4.29","4.18","4.34","4.29","4.74"]
["","Energy efficiency class","","","A+","A","A","A+","A+","A","A+","A","A+","A+","A+","A","A+","A+","A+","A+","A+","A","A+","A+","A+","A+","A+","A+"]
["","Annual energy consumption","","kWh/a","1,621","1,732","1,696","1,621","1,605","1,732","1,566","1,696","1,566","1,605","2,600","2,786","2,690","2,465","2,505","2,600","2,638","2,786","2,651","2,465","2,690","2,638","2,505","2,651","2,279","2,806","2,279","3,050","3,096","","","","3,070","3,107","3,189","3,070","3,107","2,811"]
["","ηs,h","","%","","","","","","","","","","","","","","","","","","","","","","","","","231","","","","","","","","171","169"]
["Heating capacity","Nom.","","kW","7.50 (2)","7.50 (2)","7.50 (2)","7.50 (2)","7.50 (2)","7.50 (2)","7.50 (2)","7.50 (2)","7.50 (2)","7.50 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)","13.5 (2)","13.5 (2)","13.5 (2)","13.5 (2)","13.5 (2)","","","","15.5 (2)","15.5 (2)","15.5 (2)","15.5 (2)","15.5 (2)","15.5 (2)"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Cooling capacity","Nom.","","kW","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","12.1 (1)","6.80 (1)","12.1 (1)","","","","","","","13.4 (1)","13.4 (1)"]
["Heating capacity","Nom.","","kW","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","13.5 (2)","7.50 (2)","13.5 (2)","","","","","","","15.5 (2)","15.5 (2)"]
["Space cooling","Capacity","Pdesign","kW","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","12.1","6.80","12.1","","","","","","","13.4","13.4"]
["","SEER","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","9.74","7.90","6.56","","","","","","","8.95","8.8"]
["","Annual energy consumption","","kWh/a","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","745","301","1107","","","","","","","898","914"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","9.52","4.70","9.52","","","","","","","9.52","9.52"]
["","SCOP/A","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","4.75","4.61","4.37","","","","","","","4.74","4.18"]
["","Annual energy consumption","","kWh/a","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","2806","1,427","3050","","","","","","","2811","3189"]
["Space cooling","Energy efficiency class","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","A++"]
["Space heating (Average climate)","Energy efficiency class","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","A++"]
["Energy Efficiency Range","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","","A+++ ~ D"]