{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":8,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C / RZQ-DV1"]
[]
[]
[]
[]
["","","","","FBQ71C7VEB / RZQ71D7V1B","FBQ100C7VEB / RZQ100D7V1B","FBQ125C7VEB / RZQ125D7V1B","FBQ140C7VEB / RZQ140D7V1B"]
["Cooling capacity","Nom.","","kW","7.1 (1)","10.0 (1)","12.5 (1)","13.4 (1)"]
["Piping connections","Liquid","OD","mm","9.52","9.52","9.52","9.52"]
["","Gas","OD","mm","15.9","15.9","15.9","15.9"]
["","Drain","OD","mm","26","26","26","26"]
["Nominal efficiency","EER","","","3.39","3.70","3.48","3.01"]
["","Annual energy consumption","","kWh","1,047","1,351","1,796","2,226"]
["","COP","","","3.85","4.16","3.62","3.41"]
["","Energy labeling Directive","Cooling","","A","A","A","B"]
["","","Heating","","A","A","A","B"]
["Heating capacity","Nom.","","kW","8.0 (2)","11.2 (2)","14.0 (2)","15.0 (2)"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m"]
["","","","","(3) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(3) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(3) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(3) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]