{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":23,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RZQG-L7V1/LY1"]
[]
[]
[]
[]
["","","","","FBQ100C8VEB / RZQG100L7V1B","FBQ35C8VEB / FBQ35C8VEB / RZQG71L7V1B","FBQ35C8VEB / FBQ35C8VEB / RZQG71L7Y1B9","FBQ50C8VEB / FBQ50C8VEB / RZQG100L7V1B","FBQ50C8VEB / FBQ50C8VEB / RZQG100L7Y1B","FBQ60C8VEB / FBQ60C8VEB / RZQG125L7Y1B","FBQ71C8VEB / RZQG71L7V1B","FBQ71C8VEB / RZQG71L7Y1B9","FBQ71C8VEB / RZQG71L7Y1B","FBQ100C8VEB / RZQG100L7Y1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQG100L7V1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQG100L7Y1B","FBQ125C8VEB / RZQG125L7V1B","FBQ125C8VEB / RZQG125L7Y1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQG125L7V1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQG125L7Y1B","FBQ50C8VEB / FBQ50C8VEB / FBQ50C8VEB / RZQG125L7V1B","FBQ50C8VEB / FBQ50C8VEB / FBQ50C8VEB / RZQG125L7Y1B","FBQ60C8VEB / FBQ60C8VEB / RZQG125L7V1B"]
["Cooling capacity","Nom.","","kW","9.5","","","","","","6.8","6.8","6.8 (3)","9.5","","","12.0","12.0"]
["Space cooling","SEER","","","5.61","4.30","4.30","4.30","4.30","4.30","5.61","5.61","5.61 (6)","5.61","4.30","4.30","5.61","5.61","4.30","4.30","4.30","4.30","4.30"]
["","Annual energy consumption","","kWh/a","592.692","554","554","773.256","773.256","976.744","424.242","424.242","","592.692","773.256","773.256","748.663","748.663","976.744","976.744","976.744","976.744","976.744"]
["","Capacity","Pdesign","kW","9.50","6.80","6.80","9.50","9.50","12.00","6.80","6.80","","9.50","9.50","9.50","12.00","12.00","12.00","12.00","12.00","12.00","12.00"]
["","Energy efficiency class","","","A+","C","C","C","C","C","A+","A+","","A+","C","C","A+","A+","C","C","C","C","C"]
["Space heating (Average climate)","Capacity","Pdesign","kW","11.30","6.00","6.00","10.20","10.20","12.71","6.00","6.00","","11.30","10.20","10.20","12.71","12.71","12.71","12.71","12.71","12.71","12.71"]
["","SCOP/A","","","4.25","3.40","3.40","3.80","3.80","3.40","4.01","4.01","4.01 (6)","4.25","3.80","3.80","4.05","4.05","3.40","3.40","3.40","3.40","3.40"]
["","Energy efficiency class","","","A+","A","A","A","A","A","A+","A+","","A+","A","A","A+","A+","A","A","A","A","A"]
["","Annual energy consumption","","kWh/a","3,724","2,472","2,472","3,757","3,757","5,232","2,094.763","2,094.763","","3,724","3,757","3,757","4,392","4,392","5,232","5,232","5,232","5,232","5,232"]
["Nominal efficiency","EER","","","3.89","","","","","","3.50","3.50","3.50","3.89","","","3.81","3.81"]
["","Annual energy consumption","","kWh","1,220","","","","","","970","970","970","1,220","","","1,575","1,575"]
["","COP","","","4.21","","","","","","3.65","3.65","3.65","4.21","","","3.83","3.83"]
["","Energy labeling Directive","Cooling","","A","","","","","","A","A","A","A","","","A","A"]
["","","Heating","","A","","","","","","A","A","A","A","","","A","A"]
["Heating capacity","Nom.","","kW","10.8","","","","","","7.5","7.5","7.5 (4)","10.8","","","13.5","13.5"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","","","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(1) - EER/COP according to Eurovent 2012, for use outside EU only","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Energy label: scale from A (most efficient) to G (less efficient)","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","","","","","","","","","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","","","","","","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m"]
["","","","","","","","","","","","","(5) - Annual energy consumption is according to Energy labeling directive 2002/31/EC"]
["","","","","","","","","","","","","(6) - SEER and SCOP are according to EN 14825"]
["","","","","","","","","","","","","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]