{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":14,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RZQG-L8/7V1"]
[]
[]
[]
[]
["","","","","FBQ35C8VEB / FBQ35C8VEB / RZQG71L8V1B","FBQ71C8VEB / RZQG71L8V1B","FBQ100C8VEB / RZQG100L8V1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQG100L8V1B","FBQ50C8VEB / FBQ50C8VEB / RZQG100L8V1B","FBQ125C8VEB / RZQG125L8V1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQG125L8V1B","FBQ50C8VEB / FBQ50C8VEB / FBQ50C8VEB / RZQG125L8V1B","FBQ60C8VEB / FBQ60C8VEB / RZQG125L8V1B","FBQ140C8VEB / RZQG140L7V1B"]
["Cooling capacity","Nom.","","kW","","6.8","9.5","","","12.0","","","","13.4"]
["Space cooling","SEER","","","5.10","6.11","5.80","5.10","5.10","5.81","5.10","5.10","5.10"]
["","Annual energy consumption","","kWh/a","467","389.525","573.276","652","652","722.892","824","824","824"]
["","Capacity","Pdesign","kW","6.80","6.80","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Energy efficiency class","","","A","A++","A+","A","A","A+","A","A","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","6.00","6.00","11.30","11.30","11.30","12.71","12.71","12.71","12.71"]
["","SCOP/A","","","3.80","4.01","4.61","3.80","3.80","4.21","3.80","3.80","3.80"]
["","Energy efficiency class","","","A","A+","A++","A","A","A+","A","A","A"]
["","Annual energy consumption","","kWh/a","2,211","2,094.763","3,431.67","4,163","4,163","4,226.603","4,683","4,683","4,683"]
["Nominal efficiency","EER","","","","3.50","3.89","","","3.81","","","","3.33"]
["","Annual energy consumption","","kWh","","970","1,220","","","1,575","","","","2,010"]
["","COP","","","","3.65","4.21","","","3.83","","","","3.61"]
["","Energy labeling Directive","Cooling","","","A","A","","","A"]
["","","Heating","","","A","A","","","A"]
["Heating capacity","Nom.","","kW","","7.5","10.8","","","13.5","","","","15.5"]
["Notes","","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]