{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQ-C8 / RXS-G"]
[]
[]
[]
[]
["","","","","FCQ35C8VEB / RXS35G2V1B","FCQ50C8VEB / RXS50G2V1B"]
["Cooling capacity","Nom.","","kW","3.40 (3), 5.00 (1)","5.00 (3)"]
["Nominal efficiency","EER","","","3.58","3.55"]
["","Annual energy consumption","","kWh","475","705"]
["","COP","","","3.41","3.70"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","B","A"]
["Heating capacity","Nom.","","kW","4.20 (4)","6.00 (4)"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(3) - Cooling: return air temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent refrigerant piping length 5m (horizontal)","(3) - Cooling: return air temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent refrigerant piping length 5m (horizontal)"]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]