{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":11,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQ-C8"]
[]
[]
[]
[]
["","","","","FCQ35C8VEB","FCQ50C8VEB","FCQ60C8VEB","FCQ71C8VEB","FCQ100C8VEB","FCQ125C8VEB","FCQ140C8VEB"]
["Sound pressure level","Heating","High","dBA","31","31","33","34","37","41","42"]
["","","Low","dBA","27","27","28","28","32","35","35"]
["","Cooling","Low","dBA","27","27","28","28","32","35","35"]
["","","High","dBA","31","31","33","33","37","41","41"]
["Standard Accessories","Operation manual","","","Operation manual","Operation manual","Operation manual","Operation manual","Operation manual","Operation manual","Operation manual"]
["","Installation manual","","","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual"]
["","Drain hose","","","Drain hose","Drain hose","Drain hose","Drain hose","Drain hose","Drain hose","Drain hose"]
["","Clamp for drain hose","","","Clamp for drain hose","Clamp for drain hose","Clamp for drain hose","Clamp for drain hose","Clamp for drain hose","Clamp for drain hose","Clamp for drain hose"]
["","Washer for hanger bracket","","","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket"]
["","Screws","","","Screws","Screws","Screws","Screws","Screws","Screws","Screws"]
["","Installation guide","","","Installation guide","Installation guide","Installation guide","Installation guide","Installation guide","Installation guide","Installation guide"]
["","Insulation for fitting","","","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting"]
["","Sealing pads","","","Sealing pads","Sealing pads","Sealing pads","Sealing pads","Sealing pads","Sealing pads","Sealing pads"]
["","Drain sealing pad","","","Drain sealing pad","Drain sealing pad","Drain sealing pad","Drain sealing pad","Drain sealing pad","Drain sealing pad","Drain sealing pad"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Gas","OD","mm","9.52","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Drain","","","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)"]
["Sound power level","Cooling","","dBA","49","49","51","51","54","58","58"]
["Dimensions","Unit","Width","mm","840","840","840","840","840","840","840"]
["","","Depth","mm","840","840","840","840","840","840","840"]
["","","Height","mm","204","204","204","204","246","246","246"]
["Casing","Material","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["Weight","Unit","","kg","19","19","19","21","23","23","23"]
["Decoration panel 2","Weight","","kg","5.5","5.5","5.5","5.5","5.5","5.5","5.5"]
["","Model","","","BYCQ140CW1W","BYCQ140CW1W","BYCQ140CW1W","BYCQ140CW1W","BYCQ140CW1W","BYCQ140CW1W","BYCQ140CW1W"]
["","Dimensions","Depth","mm","950","950","950","950","950","950","950"]
["","","Width","mm","950","950","950","950","950","950","950"]
["","","Height","mm","50","50","50","50","50","50","50"]
["","Colour","","","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)"]
["Decoration panel 3","Dimensions","Depth","mm","950","950","950","950","950","950","950"]
["","","Height","mm","130","130","130","130","130","130","130"]
["","","Width","mm","950","950","950","950","950","950","950"]
["","Colour","","","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)"]
["","Model","","","BYCQ140CGW1","BYCQ140CGW1","BYCQ140CGW1","BYCQ140CGW1","BYCQ140CGW1","BYCQ140CGW1","BYCQ140CGW1"]
["","Weight","","kg","11.5","11.5","11.5","11.5","11.5","11.5","11.5"]
["Decoration panel","Weight","","kg","5.5","5.5","5.5","5.5","5.5","5.5","5.5"]
["","Model","","","BYCQ140CW1","BYCQ140CW1","BYCQ140CW1","BYCQ140CW1","BYCQ140CW1","BYCQ140CW1","BYCQ140CW1"]
["","Dimensions","Height","mm","50","50","50","50","50","50","50"]
["","","Depth","mm","950","950","950","950","950","950","950"]
["","","Width","mm","950","950","950","950","950","950","950"]
["","Colour","","","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~","1~"]
["","Name","","","VE","VE","VE","VE","VE","VE","VE"]
["","Frequency","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Voltage","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","(1) - The sound pressure values are mentioned for a unit installed with rear suction.","(1) - The sound pressure values are mentioned for a unit installed with rear suction.","(1) - The sound pressure values are mentioned for a unit installed with rear suction.","(1) - The sound pressure values are mentioned for a unit installed with rear suction.","(1) - The sound pressure values are mentioned for a unit installed with rear suction.","(1) - The sound pressure values are mentioned for a unit installed with rear suction.","(1) - The sound pressure values are mentioned for a unit installed with rear suction."]
["","","","","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates.","(2) - The sound power level is an absolute value indicating the power which a sound source generates."]
["","","","","(3) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt."]
["","","","","(4) - Maximum allowable voltage range variation between phases is 2%.","(4) - Maximum allowable voltage range variation between phases is 2%.","(4) - Maximum allowable voltage range variation between phases is 2%.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","(5) - Select wire size based on the value of MCA","(5) - Select wire size based on the value of MCA","(5) - Select wire size based on the value of MCA","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","(6) - Instead of a fuse, use a circuit breaker","(6) - Instead of a fuse, use a circuit breaker","(6) - Instead of a fuse, use a circuit breaker","(6) - Select wire size based on the larger value of MCA or TOCA","(6) - Select wire size based on the larger value of MCA or TOCA","(6) - Select wire size based on the larger value of MCA or TOCA","(6) - Select wire size based on the larger value of MCA or TOCA"]
["","","","","","","","(7) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(7) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(7) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(7) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker)."]