{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":8,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-E / RZQG-L"]
[]
[]
[]
[]
["","","","","FCQG71EVEB / RZQG71LV1B","FCQG100EVEB / RZQG100LV1B","FCQG125EVEB / RZQG125LV1B","FCQG140EVEB / RZQG140LV1B"]
["Cooling capacity","Nom.","","kW","7.1 (3)","10.0 (3)","12.0 (3)","14.0 (3)"]
["Space cooling","SEER","","","4.67 (5)","4.62 (5)","4.43"]
["Nominal efficiency","EER","","","3.84","4.05","3.60","3.21"]
["","Annual energy consumption","","kWh","925","1,235","1,665","2,180"]
["","COP","","","4.71","4.71","4.24","4.01"]
["","Energy labeling Directive","Cooling","","A","A","A","A"]
["","","Heating","","A","A","A","A"]
["Heating capacity","Nom.","","kW","8.0 (4)","11.2 (4)","14.0 (4)","16 (4)"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m (horizontal)","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m (horizontal)","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m (horizontal)","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m (horizontal)"]
["","","","","(4) - Heating: indoor temp. 20°CDB, 15°CWB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal);","(4) - Heating: indoor temp. 20°CDB, 15°CWB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal);","(4) - Heating: indoor temp. 20°CDB, 15°CWB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal);","(4) - Heating: indoor temp. 20°CDB, 15°CWB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal);"]
["","","","","(5) - SEER: Pr-EN14825 - inquiry version 2010","(5) - SEER: Pr-EN14825 - inquiry version 2010","(5) - SEER: Pr-EN14825 - inquiry version 2010","(5) - All data mentioned is preliminary information"]
["","","","","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]