{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":8,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQH-D"]
[]
[]
[]
[]
["","","","","FCQH71D7VEB","FCQH100D7VEB","FCQH125D7VEB","FCQH140D7VEB"]
["Sound pressure level","Heating","High","dBA","36","45","45","45"]
["","","Low","dBA","28","32","36","38"]
["","Cooling","Low","dBA","28","32","36","38"]
["","","High","dBA","36","45","45","45"]
["Standard Accessories","Installation and operation manual","","","Installation and operation manual","Installation and operation manual","Installation and operation manual","Installation and operation manual"]
["","Drain hose","","","Drain hose","Drain hose","Drain hose","Drain hose"]
["","Clamp for drain hose","","","Clamp for drain hose","Clamp for drain hose","Clamp for drain hose","Clamp for drain hose"]
["","Washer for hanger bracket","","","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket"]
["","Screws","","","Screws","Screws","Screws","Screws"]
["","Installation guide","","","Installation guide","Installation guide","Installation guide","Installation guide"]
["","Insulation for fitting","","","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting"]
["","Sealing pad","","","Sealing pad","Sealing pad","Sealing pad","Sealing pad"]
["","Drain sealing pad","","","Drain sealing pad","Drain sealing pad","Drain sealing pad","Drain sealing pad"]
["Piping connections","Liquid","OD","mm","9.52","9.52","9.52","9.52"]
["","Gas","OD","mm","15.9","15.9","15.9","15.9"]
["","Drain","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Sound power level","Cooling","","dBA","54","62","62","62"]
["Dimensions","Unit","Width","mm","840","840","840","840"]
["","","Depth","mm","840","840","840","840"]
["","","Height","mm","246","288","288","288"]
["Casing","Material","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["Weight","Unit","","kg","23","25","25","25"]
["Decoration panel 2","Weight","","kg","5.5","5.5","5.5","5.5"]
["","Model","","","BYCQ140CW1W","BYCQ140CW1W","BYCQ140CW1W","BYCQ140CW1W"]
["","Dimensions","Depth","mm","950","950","950","950"]
["","","Width","mm","950","950","950","950"]
["","","Height","mm","50","50","50","50"]
["","Colour","","","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)"]
["Decoration panel","Weight","","kg","5.5","5.5","5.5","5.5"]
["","Model","","","BYCQ140CW1","BYCQ140CW1","BYCQ140CW1","BYCQ140CW1"]
["","Dimensions","Height","mm","50","50","50","50"]
["","","Depth","mm","950","950","950","950"]
["","","Width","mm","950","950","950","950"]
["","Colour","","","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Name","","","VE","VE","VE","VE"]
["","Frequency","","Hz","50/60","50/60","50/60","50/60"]
["","Voltage","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","(1) - The sound power level is an absolute value indicating the power which a sound source generates.","(1) - The sound power level is an absolute value indicating the power which a sound source generates.","(1) - The sound power level is an absolute value indicating the power which a sound source generates.","(1) - The sound power level is an absolute value indicating the power which a sound source generates."]
["","","","","(2) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt.","(2) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt.","(2) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt.","(2) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt."]