{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDKS-E"]
[]
[]
[]
[]
["","","","","FDKS25E7VMB","FDKS25EAVMB","FDKS35E7VMB","FDKS35EAVMB"]
["Sound pressure level","Cooling","Silent operation","dBA","29.0","29.0","29.0","29.0"]
["","","Low","dBA","31.0","31.0","31.0","31.0"]
["","","High","dBA","35.0","35.0","35.0","35.0"]
["","","Nom.","dBA","33.0","33.0","33.0","33.0"]
["Standard Accessories","Installation manual","","","1","1","1","1"]
["","Operation manual","","","1","1","1","1"]
["","Wireless remote control","","","1","","1"]
["","Batteries","","","2","2","2","2"]
["","Remote control holder","","","1","1","1","1"]
["","Fixing screw for remote control","","","2","2","2","2"]
["","Signal receiver cover kit","","","1","1","1","1"]
["","Insulation for fitting","","","1","1","1","1"]
["","Sealing pad","","","1","1","1","1"]
["","Clamp metal","","","1","1","1","1"]
["","Drain hose","","","1","1","1","1"]
["","Washer for hanger bracket","","","8","8","8","8"]
["","Sealing material","","","2","2","2","2"]
["","Clamps","","","6","6","6","6"]
["","Washer fixing plate","","","4","4","4","4"]
["","Screws for duct flanges","","","1","1","1","1"]
["","Air filter","","","1","1","1","1"]
["Sound power level","Cooling","","dBA","53.0","53.0","53.0","53.0"]
["Dimensions","Unit","Width","mm","700","700","700","700"]
["","","Depth","mm","620","620","620","620"]
["","","Height","mm","200","200","200","200"]
["Weight","Unit","","kg","21.0","21.0","21.0","21.0"]
["Fan","External static pressure","Nom.","Pa","30","30","30","30"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Name","","","VM","VM","VM","VM"]
["","Frequency","","Hz","50/60","50/60","50/60","50/60"]
["","Voltage","","V","220-240/220-230","220-240/220-230","220-240/220-230","220-240/220-230"]
["Notes","","","","(1) - SL: The silent fan level of the air flow rate setting","(1) - Sound levels are measured in an anechoic room.","(1) - SL: The silent fan level of the air flow rate setting","(1) - Sound levels are measured in an anechoic room."]
["","","","","(2) - Operating sound is based on the rear side suction inlet and ESP 40Pa. Operating sound for under side suction inlet: (operation sound for rear side suction inlet) +5dB. However, when installation to which the ESP becomes low is carried out, 5dB or more may","(2) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(2) - Operating sound is based on the rear side suction inlet and ESP 40Pa. Operating sound for under side suction inlet: (operation sound for rear side suction inlet) +5dB. However, when installation to which the ESP becomes low is carried out, 5dB or more may","(2) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings."]
["Standard Accessories","Infrared remote control","","","","1","","1"]
["Notes","","","","","(3) - Sound power level is an absolute value that a sound source generates.","","(3) - Sound power level is an absolute value that a sound source generates."]