{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-C"]
[]
[]
[]
[]
["","","","","FDXS50C7VMB","FDXS60C7VMB"]
["Sound pressure level","Heating","High","dBA","37.0","38.0"]
["","","Silent operation","dBA","31.0","32.0"]
["","","Low","dBA","33.0","34.0"]
["","Cooling","Silent operation","dBA","31.0","32.0"]
["","","Low","dBA","33.0","34.0"]
["","","High","dBA","37.0","38.0"]
["","","Nom.","dBA","35.0","36.0"]
["","Cooling","Nom.","dBA","35.0","36.0"]
["Standard Accessories","Installation manual","","","1","1"]
["","Operation manual","","","1","1"]
["","Infrared remote control","","","","1"]
["","Batteries","","","2","2"]
["","Remote control holder","","","1","1"]
["","Fixing screw for remote control","","","2","2"]
["","Signal receiver cover kit","","","1","1"]
["","Insulation for fitting","","","1","1"]
["","Sealing pad","","","1","1"]
["","Clamp metal","","","1","1"]
["","Drain hose","","","1","1"]
["","Washer for hanger bracket","","","8","8"]
["","Sealing material","","","2","2"]
["","Clamps","","","6","6"]
["","Washer fixing plate","","","4","4"]
["","Screws for duct flanges","","","1","1"]
["","Air filter","","","1","1"]
["Piping connections","Liquid","OD","mm","6.35","6.35"]
["","Gas","OD","mm","12.7","12.7"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Cooling","","dBA","55.0","56.0"]
["","Heating","","dBA","55.0","56.0"]
["Dimensions","Unit","Width","mm","900","1,100"]
["","","Depth","mm","620","620"]
["","","Height","mm","200","200"]
["Casing","Colour","","","Unpainted","Unpainted"]
["Weight","Unit","","kg","27.0","30.0"]
["Fan","External static pressure","Nom.","Pa","40","40"]
["Power supply","Phase","","","1~","1~"]
["","Name","","","VM","VM"]
["","Frequency","","Hz","50/60","50/60"]
["","Voltage","","V","220-240/220-230","220-240/220-230"]
["Notes","","","","(1) - SL: The silent fan level of the air flow rate setting","(1) - SL: The silent fan level of the air flow rate setting"]
["Standard Accessories","Wireless remote control","","","1"]