{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":8,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-E / RXS-G"]
[]
[]
[]
[]
["","","","","FDXS25E7VMB / RXS25G2V1B","FDXS25EAVMB / RXS25G2V1B","FDXS35E7VMB / RXS35G2V1B","FDXS35EAVMB / RXS35G2V1B"]
["Cooling capacity","Min.","","kW","1.3 (3)","1.3","1.4 (3)","1.4"]
["","Max.","","kW","3.0 (3)","3.0","3.8 (3)","3.8"]
["","Nom.","","kW","2.4 (3)","2.4 (1)","3.4 (3)","3.4 (1)"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.52","9.5","9.52"]
["","Drain","OD","mm","26","26","26","26"]
["Nominal efficiency","EER","","","3.48","3.48","3.12","3.12"]
["","Annual energy consumption","","kWh","345","345","545","545"]
["","COP","","","3.52","3.52","3.39","3.39"]
["","Energy labeling Directive","Cooling","","A","A","B","B"]
["","","Heating","","B","B","C","C"]
["Heating capacity","Nom.","","kW","3.2 (4)","3.2 (2)","4.0 (4)","4.0 (2)"]
["","Min.","","kW","1.3 (4)","1.3","1.4 (4)","1.4"]
["","Max.","","kW","4.5 (4)","4.5","5.0 (4)","5.0"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(5) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","(5) - SL: The silent fan level of the air flow rate setting"]
["","","","","","","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]