{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":8,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB","FFA50A2VEB","FFA60A2VEB"]
["Casing","Material","","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["Dimensions","Unit","","Height","mm","260","260","260"]
["","","","Width","mm","575","575","575"]
["","","","Depth","mm","575","575","575"]
["Weight","Unit","","","kg","16.0","17.5","17.5"]
["Fan","Air flow rate","Cooling","High","m³/min","9.0","12.0","14.5"]
["","","","Medium","m³/min","8.0","10.0","12.5"]
["","","","Low","m³/min","6.5","7.5","9.5"]
["","","Heating","High","m³/min","9.0","12.0","14.5"]
["","","","Medium","m³/min","8.0","10.0","12.5"]
["","","","Low","m³/min","6.5","7.5","9.5"]
["Sound power level","Cooling","","","dBA","48","56","60"]
["Sound pressure level","Cooling","","High","dBA","31.0","39.0","43.0"]
["","","","Medium","dBA","28.5","34.0","40.0"]
["","","","Low","dBA","25.0","27.0","32.0"]
["","Heating","","High","dBA","31.0","39.0","43.0"]
["","","","Medium","dBA","28.5","34.0","40.0"]
["","","","Low","dBA","25.0","27.0","32.0"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.52","12.70","12.70"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Decoration panel","Model","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Colour","","","","White (N9.5)","White (N9.5)","White (N9.5)"]
["","Dimensions","","Height","mm","46","46","46"]
["","","","Width","mm","620","620","620"]
["","","","Depth","mm","620","620","620"]
["","Weight","","","kg","2.8","2.8","2.8"]
["Decoration panel 2","Model","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","Colour","","","","Silver","Silver","Silver"]
["","Dimensions","","Height","mm","46","46","46"]
["","","","Width","mm","620","620","620"]
["","","","Depth","mm","620","620","620"]
["","Weight","","","kg","2.8","2.8","2.8"]
["Decoration panel 3","Model","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","Colour","","","","White (RAL9010)","White (RAL9010)","White (RAL9010)"]
["","Dimensions","","Height","mm","55","55","55"]
["","","","Width","mm","700","700","700"]
["","","","Depth","mm","700","700","700"]
["","Weight","","","kg","2.7","2.7","2.7"]
["Decoration panel 4","Model","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Colour","","","","White (RAL9010)","White (RAL9010)","White (RAL9010)"]
["","Dimensions","","Height","mm","55","55","55"]
["","","","Width","mm","700","700","700"]
["","","","Depth","mm","700","700","700"]
["","Weight","","","kg","2.7","2.7","2.7"]
["Control systems","Infrared remote control","","","","BRC7EB530W (standard panel), BRC7F530W (white panel), BRC7F530S (grey panel)","BRC7EB530W (standard panel), BRC7F530W (white panel), BRC7F530S (grey panel)","BRC7EB530W (standard panel), BRC7F530W (white panel), BRC7F530S (grey panel)"]
["","Wired remote control","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Standard Accessories","Washer for hanger bracket","","","","8","8","8"]
["","Thermal insulation tube","","","","2","2","2"]
["","Hose band","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Installation and operation manual","","","","1","1","1"]
["","Screws","","","","4","4","4"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","7","7","7"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]