{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":10,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RXM-R"]
[]
[]
[]
[]
["","","","","FFA25A2VEB9 / RXM25R5V1B","FFA35A2VEB9 / RXM35R5V1B","FFA50A2VEB9 / RXM50R5V1B","FFA50A2VEB9 / RXM50R2V1B","FFA60A2VEB9 / RXM60R5V1B","FFA60A2VEB9 / RXM60R2V1B"]
["Cooling capacity","Nom.","","kW","2.50","3.40","5.00","5.00","5.70","5.70"]
["Heating capacity","Nom.","","kW","3.20","4.20","5.80","5.80","7.00","7.00"]
["Nominal efficiency","Annual energy consumption","","kWh","273","446","772","772","931","931"]
["","COP","","","3.90","3.50","3.49","3.49","3.41","3.41"]
["","EER","","","4.57","3.81","3.24","3.24","3.05","3.05"]
["","Energy labeling Directive","Cooling","","A","A","A","A","B","B"]
["","","Heating","","A","B","B","B","B","B"]
["Space cooling","Annual energy consumption","","kWh/a","142","186","293","293","346","346"]
["","Energy efficiency class","","","A++","A++","A+","A+","A+","A+"]
["","Capacity","Pdesign","kW","2.50","3.40","5.00","5.00","5.70","5.70"]
["","SEER","","","6.17","6.38","5.98","5.98","5.76","5.76"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","762","1,058","1,378","1,378","1,373","1,373"]
["","Capacity","Pdesign","kW","2.31","3.10","3.84","3.84","3.96","3.96"]
["","Energy efficiency class","","","A+","A+","A","A","A+","A+"]
["","Pdh Heating capacity at -10°","","kW","2.03","","3.40","3.40","3.50","3.50"]
["","SCOP/A","","","4.24","4.10","3.90","3.90","4.04","4.04"]
["Notes","","","","(1) - See separate drawing for electrical data","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - See separate drawing for operation range","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]