{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-B9V / RXS-J"]
[]
[]
[]
[]
["","","","","FFQ50B9V1B / RXS50J2V1B"]
["Cooling capacity","Min.","","kW","0.9"]
["","Max.","","kW","5.6"]
["","Nom.","","kW","4.7 (3)"]
["Piping connections","Liquid","OD","mm","6.35"]
["","Gas","OD","mm","12.7"]
["","Drain","OD","mm","VP20 (External dia.26, Internal dia. 20)"]
["Nominal efficiency","EER","","","2.61"]
["","Annual energy consumption","","kWh","900"]
["","COP","","","2.81"]
["","Energy labeling Directive","Cooling","","D"]
["","","Heating","","D"]
["Heating capacity","Nom.","","kW","5.5 (4)"]
["","Min.","","kW","0.9"]
["","Max.","","kW","7.0"]
["Notes","","","","(1) - Energy label: scale from A (most efficient) to G (less efficient)"]
["","","","","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(5) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected."]
["","","","","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]