{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":12,"n_cols":4,"rows_kept":12,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-BV / RKS-J"]
[]
[]
[]
[]
["","FFQ25B8V1B / RKS25J2V1B (Preliminary)","FFQ35B8V1B / RKS35J2V1B (Preliminary)","FFQ50B8V1B / RKS50J2V1B (Preliminary)"]
["Notes","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)","(1) - Energy label: scale from A (most efficient) to G (less efficient)"]
["Notes","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)","(2) - Annual energy consumption: based on average use of 500 running hours per year at full load (nominal conditions)"]
["Notes","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["Notes","(4) - All data mentioned is preliminary information","(4) - All data mentioned is preliminary information","(4) - All data mentioned is preliminary information"]
["Notes","(5) - All data mentioned is preliminary information","(5) - All data mentioned is preliminary information","(5) - All data mentioned is preliminary information"]
["Notes","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(6) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]