{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":9,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-BV"]
[]
[]
[]
[]
["","","","","","FFQ25B8V1B","FFQ35B8V1B","FFQ50B8V1B","FFQ60B8V1B"]
["Dimensions","Unit","","Height","mm","286","286","286","286"]
["","","","Width","mm","575","575","575","575"]
["","","","Depth","mm","575","575","575","575"]
["Weight","Unit","","","kg","17.5","17.5","17.5","17.5"]
["Fan","Air flow rate","Cooling","High","m³/min","9.0","10.0","12.0","15.0"]
["","","","Low","m³/min","6.5","6.5","8.0","10.0"]
["","","Heating","High","m³/min","9.0","10.0","12.0","15.0"]
["","","","Low","m³/min","6.5","6.5","8.0","10.0"]
["Sound power level","Cooling","","","dBA","46.5","49.0","53.0","58.0"]
["Sound pressure level","Cooling","","High","dBA","29.5","32.0","36.0","41.0"]
["","","","Low","dBA","24.5","25.0","27.0","32.0"]
["","Heating","","High","dBA","29.5","32.0","36.0","41.0"]
["","","","Low","dBA","24.5","25.0","27.0","32.0"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.52","9.52","12.7","12.7"]
["","Drain","","","","26","26","26","26"]
["Decoration panel","Model","","","","BYFQ60BAW1","BYFQ60BAW1","BYFQ60BAW1","BYFQ60BAW1"]
["","Colour","","","","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)"]
["","Dimensions","","Height","mm","55","55","55","55"]
["","","","Width","mm","700","700","700","700"]
["","","","Depth","mm","700","700","700","700"]
["","Weight","","","kg","2.7","2.7","2.7","2.7"]
["Standard Accessories","Installation and operation manual","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Clamp for drain hose","","","","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8"]
["","Big clamp","","","","6","6","6","6"]
["","Small clamp","","","","1","1","1","1"]
["","Paper pattern for installation","","","","1","1","1","1"]
["","Screws","","","","4","4","4","4"]
["","Washer fixing plate","","","","4","4","4","4"]
["","Insulation for fitting for gas pipe","","","","1","1","1","1"]
["","Insulation for fitting for liquid pipe","","","","1","1","1","1"]
["","Sealing pad (large)","","","","1","1","1","1"]
["","Sealing pad (small)","","","","1","1","1","1"]
["","Sealing material","","","","2","2","2","2"]
["Power supply","Name","","","","V1","V1","V1","V1"]
["","Phase","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","230","230","230","230"]
["Notes","","","","","(1) - Sound values are measured in an anechoic room.","(1) - Sound values are measured in an anechoic room.","(1) - Sound values are measured in an anechoic room.","(1) - Sound values are measured in an anechoic room."]
["","","","","","(2) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(2) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(2) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(2) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings."]
["","","","","","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates."]